Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    startup_stm32f103xe.o(RESET) refers to startup_stm32f103xe.o(STACK) for __initial_sp
    startup_stm32f103xe.o(RESET) refers to startup_stm32f103xe.o(.text) for Reset_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.NMI_Handler) for NMI_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.HardFault_Handler) for HardFault_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.MemManage_Handler) for MemManage_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.BusFault_Handler) for BusFault_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.UsageFault_Handler) for UsageFault_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.SVC_Handler) for SVC_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.DebugMon_Handler) for DebugMon_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.PendSV_Handler) for PendSV_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.SysTick_Handler) for SysTick_Handler
    startup_stm32f103xe.o(RESET) refers to stm32f1xx_it.o(i.EXTI0_IRQHandler) for EXTI0_IRQHandler
    startup_stm32f103xe.o(.text) refers to system_stm32f1xx.o(i.SystemInit) for SystemInit
    startup_stm32f103xe.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    main.o(i.MX_GPIO_Init) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    main.o(i.MX_GPIO_Init) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    main.o(i.MX_GPIO_Init) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    main.o(i.MX_GPIO_Init) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    main.o(i.MX_SPI1_Init) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_Init) for HAL_SPI_Init
    main.o(i.MX_SPI1_Init) refers to main.o(.bss) for .bss
    main.o(i.SystemClock_Config) refers to memseta.o(.text) for __aeabi_memclr4
    main.o(i.SystemClock_Config) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig) for HAL_RCC_OscConfig
    main.o(i.SystemClock_Config) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig) for HAL_RCC_ClockConfig
    main.o(i.fputc) refers to stm32f1xx_hal_uart.o(i.HAL_UART_Transmit) for HAL_UART_Transmit
    main.o(i.fputc) refers to main.o(.bss) for .bss
    main.o(i.main) refers to stm32f1xx_hal.o(i.HAL_Init) for HAL_Init
    main.o(i.main) refers to main.o(i.SystemClock_Config) for SystemClock_Config
    main.o(i.main) refers to main.o(i.MX_GPIO_Init) for MX_GPIO_Init
    main.o(i.main) refers to main.o(i.MX_SPI1_Init) for MX_SPI1_Init
    main.o(i.main) refers to stm32f1xx_hal_uart.o(i.HAL_UART_Init) for HAL_UART_Init
    main.o(i.main) refers to printf8.o(i.__0printf$8) for __2printf
    main.o(i.main) refers to test.o(i.LoRa_Init) for LoRa_Init
    main.o(i.main) refers to test.o(i.LoRa_Test_Main) for LoRa_Test_Main
    main.o(i.main) refers to main.o(.bss) for .bss
    stm32f1xx_it.o(i.EXTI0_IRQHandler) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler) for HAL_GPIO_EXTI_IRQHandler
    stm32f1xx_it.o(i.SysTick_Handler) refers to stm32f1xx_hal.o(i.HAL_IncTick) for HAL_IncTick
    stm32f1xx_hal_msp.o(i.HAL_SPI_MspDeInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_DeInit) for HAL_GPIO_DeInit
    stm32f1xx_hal_msp.o(i.HAL_SPI_MspInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32f1xx_hal_msp.o(i.HAL_UART_MspDeInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_DeInit) for HAL_GPIO_DeInit
    stm32f1xx_hal_msp.o(i.HAL_UART_MspInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f1xx_hal_spi.o(i.SPI_AbortTx_ISR) for SPI_AbortTx_ISR
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f1xx_hal_spi.o(i.SPI_AbortRx_ISR) for SPI_AbortRx_ISR
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback) for HAL_SPI_AbortCpltCallback
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f1xx_hal_spi.o(i.SPI_AbortTx_ISR) for SPI_AbortTx_ISR
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f1xx_hal_spi.o(i.SPI_AbortRx_ISR) for SPI_AbortRx_ISR
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f1xx_hal_spi.o(i.SPI_DMATxAbortCallback) for SPI_DMATxAbortCallback
    stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f1xx_hal_spi.o(i.SPI_DMARxAbortCallback) for SPI_DMARxAbortCallback
    stm32f1xx_hal_spi.o(i.HAL_SPI_DMAStop) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f1xx_hal_spi.o(i.HAL_SPI_DeInit) refers to stm32f1xx_hal_msp.o(i.HAL_SPI_MspDeInit) for HAL_SPI_MspDeInit
    stm32f1xx_hal_spi.o(i.HAL_SPI_IRQHandler) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f1xx_hal_spi.o(i.HAL_SPI_IRQHandler) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.HAL_SPI_IRQHandler) refers to stm32f1xx_hal_spi.o(i.SPI_DMAAbortOnError) for SPI_DMAAbortOnError
    stm32f1xx_hal_spi.o(i.HAL_SPI_Init) refers to stm32f1xx_hal_msp.o(i.HAL_SPI_MspInit) for HAL_SPI_MspInit
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive) for HAL_SPI_TransmitReceive
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTransaction) for SPI_EndRxTransaction
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) for HAL_SPI_TransmitReceive_DMA
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt) for SPI_DMAHalfReceiveCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt) for SPI_DMAReceiveCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAError) for SPI_DMAError
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_IT) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) for HAL_SPI_TransmitReceive_IT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_IT) refers to stm32f1xx_hal_spi.o(i.SPI_RxISR_16BIT) for SPI_RxISR_16BIT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_IT) refers to stm32f1xx_hal_spi.o(i.SPI_RxISR_8BIT) for SPI_RxISR_8BIT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt) for SPI_DMAHalfTransmitReceiveCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) for SPI_DMATransmitReceiveCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAError) for SPI_DMAError
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt) for SPI_DMAHalfReceiveCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt) for SPI_DMAReceiveCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f1xx_hal_spi.o(i.SPI_2linesRxISR_16BIT) for SPI_2linesRxISR_16BIT
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f1xx_hal_spi.o(i.SPI_2linesTxISR_16BIT) for SPI_2linesTxISR_16BIT
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f1xx_hal_spi.o(i.SPI_2linesRxISR_8BIT) for SPI_2linesRxISR_8BIT
    stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f1xx_hal_spi.o(i.SPI_2linesTxISR_8BIT) for SPI_2linesTxISR_8BIT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt) for SPI_DMAHalfTransmitCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt) for SPI_DMATransmitCplt
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f1xx_hal_spi.o(i.SPI_DMAError) for SPI_DMAError
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_IT) refers to stm32f1xx_hal_spi.o(i.SPI_TxISR_16BIT) for SPI_TxISR_16BIT
    stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_IT) refers to stm32f1xx_hal_spi.o(i.SPI_TxISR_8BIT) for SPI_TxISR_8BIT
    stm32f1xx_hal_spi.o(i.SPI_2linesRxISR_16BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f1xx_hal_spi.o(i.SPI_2linesRxISR_8BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f1xx_hal_spi.o(i.SPI_2linesTxISR_16BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f1xx_hal_spi.o(i.SPI_2linesTxISR_8BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f1xx_hal_spi.o(i.SPI_AbortRx_ISR) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TxRxCpltCallback) for HAL_SPI_TxRxCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_RxCpltCallback) for HAL_SPI_RxCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTransaction) for SPI_EndRxTransaction
    stm32f1xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_RxCpltCallback) for HAL_SPI_RxCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TxCpltCallback) for HAL_SPI_TxCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_spi.o(i.SPI_DMAAbortOnError) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_DMAError) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_RxHalfCpltCallback) for HAL_SPI_RxHalfCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TxHalfCpltCallback) for HAL_SPI_TxHalfCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TxRxHalfCpltCallback) for HAL_SPI_TxRxHalfCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTransaction) for SPI_EndRxTransaction
    stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_RxCpltCallback) for HAL_SPI_RxCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMARxAbortCallback) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_DMARxAbortCallback) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f1xx_hal_spi.o(i.SPI_DMARxAbortCallback) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback) for HAL_SPI_AbortCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TxCpltCallback) for HAL_SPI_TxCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TxRxCpltCallback) for HAL_SPI_TxRxCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMATxAbortCallback) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback) for HAL_SPI_AbortCpltCallback
    stm32f1xx_hal_spi.o(i.SPI_DMATxAbortCallback) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_spi.o(i.SPI_EndRxTransaction) refers to stm32f1xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction) refers to stm32f1xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f1xx_hal_spi.o(i.SPI_RxISR_16BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseRx_ISR) for SPI_CloseRx_ISR
    stm32f1xx_hal_spi.o(i.SPI_RxISR_8BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseRx_ISR) for SPI_CloseRx_ISR
    stm32f1xx_hal_spi.o(i.SPI_TxISR_16BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR) for SPI_CloseTx_ISR
    stm32f1xx_hal_spi.o(i.SPI_TxISR_8BIT) refers to stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR) for SPI_CloseTx_ISR
    stm32f1xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal.o(i.HAL_DeInit) refers to stm32f1xx_hal.o(i.HAL_MspDeInit) for HAL_MspDeInit
    stm32f1xx_hal.o(i.HAL_Delay) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal.o(i.HAL_Delay) refers to stm32f1xx_hal.o(.data) for .data
    stm32f1xx_hal.o(i.HAL_GetTick) refers to stm32f1xx_hal.o(.data) for .data
    stm32f1xx_hal.o(i.HAL_GetTickFreq) refers to stm32f1xx_hal.o(.data) for .data
    stm32f1xx_hal.o(i.HAL_GetTickPrio) refers to stm32f1xx_hal.o(.data) for .data
    stm32f1xx_hal.o(i.HAL_IncTick) refers to stm32f1xx_hal.o(.data) for .data
    stm32f1xx_hal.o(i.HAL_Init) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping) for HAL_NVIC_SetPriorityGrouping
    stm32f1xx_hal.o(i.HAL_Init) refers to stm32f1xx_hal.o(i.HAL_InitTick) for HAL_InitTick
    stm32f1xx_hal.o(i.HAL_Init) refers to stm32f1xx_hal_msp.o(i.HAL_MspInit) for HAL_MspInit
    stm32f1xx_hal.o(i.HAL_InitTick) refers to stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config) for HAL_SYSTICK_Config
    stm32f1xx_hal.o(i.HAL_InitTick) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    stm32f1xx_hal.o(i.HAL_InitTick) refers to stm32f1xx_hal.o(.data) for .data
    stm32f1xx_hal.o(i.HAL_InitTick) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal.o(i.HAL_SetTickFreq) refers to stm32f1xx_hal.o(i.HAL_InitTick) for HAL_InitTick
    stm32f1xx_hal.o(i.HAL_SetTickFreq) refers to stm32f1xx_hal.o(.data) for .data
    stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32f1xx_hal.o(i.HAL_InitTick) for HAL_InitTick
    stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to system_stm32f1xx.o(.constdata) for AHBPrescTable
    stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32f1xx_hal.o(.data) for uwTickPrio
    stm32f1xx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32f1xx_hal.o(i.HAL_InitTick) for HAL_InitTick
    stm32f1xx_hal_rcc.o(i.HAL_RCC_DeInit) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_rcc.o(i.HAL_RCC_DeInit) refers to stm32f1xx_hal.o(.data) for uwTickPrio
    stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) refers to system_stm32f1xx.o(.constdata) for APBPrescTable
    stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) refers to system_stm32f1xx.o(.constdata) for APBPrescTable
    stm32f1xx_hal_rcc.o(i.HAL_RCC_MCOConfig) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32f1xx_hal_rcc.o(i.HAL_RCC_NMI_IRQHandler) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_CSSCallback) for HAL_RCC_CSSCallback
    stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to system_stm32f1xx.o(.data) for SystemCoreClock
    stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) for HAL_RCC_GetPCLK2Freq
    stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler) refers to sx126x-board.o(i.HAL_GPIO_EXTI_Callback) for HAL_GPIO_EXTI_Callback
    stm32f1xx_hal_dma.o(i.HAL_DMA_PollForTransfer) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_dma.o(i.HAL_DMA_Start) refers to stm32f1xx_hal_dma.o(i.DMA_SetConfig) for DMA_SetConfig
    stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT) refers to stm32f1xx_hal_dma.o(i.DMA_SetConfig) for DMA_SetConfig
    stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority) refers to stm32f1xx_hal_cortex.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config) refers to stm32f1xx_hal_cortex.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler) refers to stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Callback) for HAL_SYSTICK_Callback
    stm32f1xx_hal_pwr.o(i.HAL_PWR_EnterSTOPMode) refers to stm32f1xx_hal_pwr.o(i.PWR_OverloadWfe) for PWR_OverloadWfe
    stm32f1xx_hal_pwr.o(i.HAL_PWR_PVD_IRQHandler) refers to stm32f1xx_hal_pwr.o(i.HAL_PWR_PVDCallback) for HAL_PWR_PVDCallback
    stm32f1xx_hal_flash.o(i.FLASH_Program_HalfWord) refers to stm32f1xx_hal_flash.o(.bss) for .bss
    stm32f1xx_hal_flash.o(i.FLASH_SetErrorCode) refers to stm32f1xx_hal_flash.o(.bss) for .bss
    stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) refers to stm32f1xx_hal_flash.o(i.FLASH_SetErrorCode) for FLASH_SetErrorCode
    stm32f1xx_hal_flash.o(i.HAL_FLASH_GetError) refers to stm32f1xx_hal_flash.o(.bss) for .bss
    stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f1xx_hal_flash.o(i.FLASH_SetErrorCode) for FLASH_SetErrorCode
    stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f1xx_hal_flash.o(i.HAL_FLASH_OperationErrorCallback) for HAL_FLASH_OperationErrorCallback
    stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f1xx_hal_flash.o(i.FLASH_Program_HalfWord) for FLASH_Program_HalfWord
    stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f1xx_hal_flash.o(i.HAL_FLASH_EndOfOperationCallback) for HAL_FLASH_EndOfOperationCallback
    stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_PageErase) for FLASH_PageErase
    stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f1xx_hal_flash.o(.bss) for .bss
    stm32f1xx_hal_flash.o(i.HAL_FLASH_OB_Launch) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_SystemReset) for HAL_NVIC_SystemReset
    stm32f1xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f1xx_hal_flash.o(i.HAL_FLASH_Program) refers to llushr.o(.text) for __aeabi_llsr
    stm32f1xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f1xx_hal_flash.o(i.FLASH_Program_HalfWord) for FLASH_Program_HalfWord
    stm32f1xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f1xx_hal_flash.o(.bss) for .bss
    stm32f1xx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32f1xx_hal_flash.o(i.FLASH_Program_HalfWord) for FLASH_Program_HalfWord
    stm32f1xx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32f1xx_hal_flash.o(.bss) for .bss
    stm32f1xx_hal_flash_ex.o(i.FLASH_MassErase) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP) refers to stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP) refers to stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBErase) for HAL_FLASHEx_OBErase
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP) refers to stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP) refers to stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBErase) for HAL_FLASHEx_OBErase
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig) refers to stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f1xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.FLASH_PageErase) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_MassErase) for FLASH_MassErase
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_PageErase) for FLASH_PageErase
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_PageErase) for FLASH_PageErase
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_MassErase) for FLASH_MassErase
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBErase) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_OB_GetRDP) for FLASH_OB_GetRDP
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBErase) refers to stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBErase) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig) for FLASH_OB_RDP_LevelConfig
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBErase) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_OB_GetRDP) for FLASH_OB_GetRDP
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP) for FLASH_OB_DisableWRP
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP) for FLASH_OB_EnableWRP
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f1xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig) for FLASH_OB_RDP_LevelConfig
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f1xx_hal_flash.o(.bss) for pFlash
    stm32f1xx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32f1xx_hal_msp.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f1xx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32f1xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f1xx_hal_uart.o(i.HAL_LIN_Init) refers to stm32f1xx_hal_msp.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f1xx_hal_uart.o(i.HAL_LIN_Init) refers to stm32f1xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f1xx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32f1xx_hal_msp.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f1xx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32f1xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f1xx_hal_uart.o(i.HAL_UARTEx_ReceiveToIdle) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_uart.o(i.HAL_UARTEx_ReceiveToIdle_DMA) refers to stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA) for UART_Start_Receive_DMA
    stm32f1xx_hal_uart.o(i.HAL_UARTEx_ReceiveToIdle_IT) refers to stm32f1xx_hal_uart.o(i.UART_Start_Receive_IT) for UART_Start_Receive_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_Abort) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f1xx_hal_uart.o(i.HAL_UART_Abort) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceive) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceive) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceive_IT) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceive_IT) refers to stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceiveCpltCallback) for HAL_UART_AbortReceiveCpltCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceive_IT) refers to stm32f1xx_hal_uart.o(i.UART_DMARxOnlyAbortCallback) for UART_DMARxOnlyAbortCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmit) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmit) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmit_IT) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmit_IT) refers to stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmitCpltCallback) for HAL_UART_AbortTransmitCpltCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmit_IT) refers to stm32f1xx_hal_uart.o(i.UART_DMATxOnlyAbortCallback) for UART_DMATxOnlyAbortCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32f1xx_hal_uart.o(i.HAL_UART_AbortCpltCallback) for HAL_UART_AbortCpltCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32f1xx_hal_uart.o(i.UART_DMATxAbortCallback) for UART_DMATxAbortCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_Abort_IT) refers to stm32f1xx_hal_uart.o(i.UART_DMARxAbortCallback) for UART_DMARxAbortCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f1xx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32f1xx_hal_uart.o(i.UART_EndTxTransfer) for UART_EndTxTransfer
    stm32f1xx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32f1xx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32f1xx_hal_uart.o(i.HAL_UART_DeInit) refers to stm32f1xx_hal_msp.o(i.HAL_UART_MspDeInit) for HAL_UART_MspDeInit
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_uart.o(i.UART_Receive_IT) for UART_Receive_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_uart.o(i.HAL_UART_TxCpltCallback) for HAL_UART_TxCpltCallback
    stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError) for UART_DMAAbortOnError
    stm32f1xx_hal_uart.o(i.HAL_UART_Init) refers to stm32f1xx_hal_msp.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f1xx_hal_uart.o(i.HAL_UART_Init) refers to stm32f1xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f1xx_hal_uart.o(i.HAL_UART_Receive) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_uart.o(i.HAL_UART_Receive) refers to stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32f1xx_hal_uart.o(i.HAL_UART_Receive_DMA) refers to stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA) for UART_Start_Receive_DMA
    stm32f1xx_hal_uart.o(i.HAL_UART_Receive_IT) refers to stm32f1xx_hal_uart.o(i.UART_Start_Receive_IT) for UART_Start_Receive_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_Transmit) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f1xx_hal_uart.o(i.HAL_UART_Transmit) refers to stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32f1xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f1xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f1xx_hal_uart.o(i.UART_DMATransmitCplt) for UART_DMATransmitCplt
    stm32f1xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f1xx_hal_uart.o(i.UART_DMATxHalfCplt) for UART_DMATxHalfCplt
    stm32f1xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f1xx_hal_uart.o(i.UART_DMAError) for UART_DMAError
    stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError) refers to stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32f1xx_hal_uart.o(i.UART_DMAError) refers to stm32f1xx_hal_uart.o(i.UART_EndTxTransfer) for UART_EndTxTransfer
    stm32f1xx_hal_uart.o(i.UART_DMAError) refers to stm32f1xx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32f1xx_hal_uart.o(i.UART_DMAError) refers to stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32f1xx_hal_uart.o(i.UART_DMAReceiveCplt) refers to stm32f1xx_hal_uart.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32f1xx_hal_uart.o(i.UART_DMAReceiveCplt) refers to stm32f1xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32f1xx_hal_uart.o(i.UART_DMARxAbortCallback) refers to stm32f1xx_hal_uart.o(i.HAL_UART_AbortCpltCallback) for HAL_UART_AbortCpltCallback
    stm32f1xx_hal_uart.o(i.UART_DMARxHalfCplt) refers to stm32f1xx_hal_uart.o(i.HAL_UART_RxHalfCpltCallback) for HAL_UART_RxHalfCpltCallback
    stm32f1xx_hal_uart.o(i.UART_DMARxHalfCplt) refers to stm32f1xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32f1xx_hal_uart.o(i.UART_DMARxOnlyAbortCallback) refers to stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceiveCpltCallback) for HAL_UART_AbortReceiveCpltCallback
    stm32f1xx_hal_uart.o(i.UART_DMATransmitCplt) refers to stm32f1xx_hal_uart.o(i.HAL_UART_TxCpltCallback) for HAL_UART_TxCpltCallback
    stm32f1xx_hal_uart.o(i.UART_DMATxAbortCallback) refers to stm32f1xx_hal_uart.o(i.HAL_UART_AbortCpltCallback) for HAL_UART_AbortCpltCallback
    stm32f1xx_hal_uart.o(i.UART_DMATxHalfCplt) refers to stm32f1xx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback) for HAL_UART_TxHalfCpltCallback
    stm32f1xx_hal_uart.o(i.UART_DMATxOnlyAbortCallback) refers to stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmitCpltCallback) for HAL_UART_AbortTransmitCpltCallback
    stm32f1xx_hal_uart.o(i.UART_Receive_IT) refers to stm32f1xx_hal_uart.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32f1xx_hal_uart.o(i.UART_Receive_IT) refers to stm32f1xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback) for HAL_UARTEx_RxEventCallback
    stm32f1xx_hal_uart.o(i.UART_SetConfig) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) for HAL_RCC_GetPCLK2Freq
    stm32f1xx_hal_uart.o(i.UART_SetConfig) refers to stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) for HAL_RCC_GetPCLK1Freq
    stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32f1xx_hal_uart.o(i.UART_DMAReceiveCplt) for UART_DMAReceiveCplt
    stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32f1xx_hal_uart.o(i.UART_DMARxHalfCplt) for UART_DMARxHalfCplt
    stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA) refers to stm32f1xx_hal_uart.o(i.UART_DMAError) for UART_DMAError
    stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    system_stm32f1xx.o(i.SystemCoreClockUpdate) refers to system_stm32f1xx.o(.data) for .data
    system_stm32f1xx.o(i.SystemCoreClockUpdate) refers to system_stm32f1xx.o(.constdata) for .constdata
    sx126x-board.o(i.HAL_GPIO_EXTI_Callback) refers to sx126x-board.o(.data) for .data
    sx126x-board.o(i.SX126xDbgPinRxWrite) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xDbgPinTxWrite) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xGetDio1PinState) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin) for HAL_GPIO_ReadPin
    sx126x-board.o(i.SX126xGetOperatingMode) refers to sx126x-board.o(.data) for .data
    sx126x-board.o(i.SX126xIoDbgInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xIoDbgInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    sx126x-board.o(i.SX126xIoInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xIoInit) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    sx126x-board.o(i.SX126xIoIrqInit) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    sx126x-board.o(i.SX126xIoIrqInit) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    sx126x-board.o(i.SX126xIoIrqInit) refers to stm32f1xx_hal_cortex.o(i.HAL_NVIC_DisableIRQ) for HAL_NVIC_DisableIRQ
    sx126x-board.o(i.SX126xIoIrqInit) refers to sx126x-board.o(.data) for .data
    sx126x-board.o(i.SX126xIoRfSwitchInit) refers to sx126x.o(i.SX126xSetDio2AsRfSwitchCtrl) for SX126xSetDio2AsRfSwitchCtrl
    sx126x-board.o(i.SX126xReadBuffer) refers to sx126x.o(i.SX126xCheckDeviceReady) for SX126xCheckDeviceReady
    sx126x-board.o(i.SX126xReadBuffer) refers to memseta.o(.text) for __aeabi_memclr
    sx126x-board.o(i.SX126xReadBuffer) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xReadBuffer) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive) for HAL_SPI_TransmitReceive
    sx126x-board.o(i.SX126xReadBuffer) refers to memcpya.o(.text) for __aeabi_memcpy
    sx126x-board.o(i.SX126xReadBuffer) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x-board.o(i.SX126xReadBuffer) refers to sx126x-board.o(.bss) for .bss
    sx126x-board.o(i.SX126xReadBuffer) refers to main.o(.bss) for hspi1
    sx126x-board.o(i.SX126xReadCommand) refers to sx126x.o(i.SX126xCheckDeviceReady) for SX126xCheckDeviceReady
    sx126x-board.o(i.SX126xReadCommand) refers to memseta.o(.text) for __aeabi_memclr
    sx126x-board.o(i.SX126xReadCommand) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xReadCommand) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive) for HAL_SPI_TransmitReceive
    sx126x-board.o(i.SX126xReadCommand) refers to memcpya.o(.text) for __aeabi_memcpy
    sx126x-board.o(i.SX126xReadCommand) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x-board.o(i.SX126xReadCommand) refers to sx126x-board.o(.bss) for .bss
    sx126x-board.o(i.SX126xReadCommand) refers to main.o(.bss) for hspi1
    sx126x-board.o(i.SX126xReadRegister) refers to sx126x-board.o(i.SX126xReadRegisters) for SX126xReadRegisters
    sx126x-board.o(i.SX126xReadRegisters) refers to sx126x.o(i.SX126xCheckDeviceReady) for SX126xCheckDeviceReady
    sx126x-board.o(i.SX126xReadRegisters) refers to memseta.o(.text) for __aeabi_memclr
    sx126x-board.o(i.SX126xReadRegisters) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xReadRegisters) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive) for HAL_SPI_TransmitReceive
    sx126x-board.o(i.SX126xReadRegisters) refers to memcpya.o(.text) for __aeabi_memcpy
    sx126x-board.o(i.SX126xReadRegisters) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x-board.o(i.SX126xReadRegisters) refers to sx126x-board.o(.bss) for .bss
    sx126x-board.o(i.SX126xReadRegisters) refers to main.o(.bss) for hspi1
    sx126x-board.o(i.SX126xReset) refers to timer.o(i.DelayMs) for DelayMs
    sx126x-board.o(i.SX126xReset) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xSetOperatingMode) refers to sx126x-board.o(i.SX126xDbgPinTxWrite) for SX126xDbgPinTxWrite
    sx126x-board.o(i.SX126xSetOperatingMode) refers to sx126x-board.o(i.SX126xDbgPinRxWrite) for SX126xDbgPinRxWrite
    sx126x-board.o(i.SX126xSetOperatingMode) refers to sx126x-board.o(.data) for .data
    sx126x-board.o(i.SX126xSetRfTxPower) refers to sx126x.o(i.SX126xSetTxParams) for SX126xSetTxParams
    sx126x-board.o(i.SX126xWaitOnBusy) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin) for HAL_GPIO_ReadPin
    sx126x-board.o(i.SX126xWakeup) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xWakeup) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit) for HAL_SPI_Transmit
    sx126x-board.o(i.SX126xWakeup) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x-board.o(i.SX126xWakeup) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x-board.o(i.SX126xWakeup) refers to sx126x-board.o(.bss) for .bss
    sx126x-board.o(i.SX126xWakeup) refers to main.o(.bss) for hspi1
    sx126x-board.o(i.SX126xWriteBuffer) refers to sx126x.o(i.SX126xCheckDeviceReady) for SX126xCheckDeviceReady
    sx126x-board.o(i.SX126xWriteBuffer) refers to memcpya.o(.text) for __aeabi_memcpy
    sx126x-board.o(i.SX126xWriteBuffer) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xWriteBuffer) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit) for HAL_SPI_Transmit
    sx126x-board.o(i.SX126xWriteBuffer) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x-board.o(i.SX126xWriteBuffer) refers to sx126x-board.o(.bss) for .bss
    sx126x-board.o(i.SX126xWriteBuffer) refers to main.o(.bss) for hspi1
    sx126x-board.o(i.SX126xWriteCommand) refers to sx126x.o(i.SX126xCheckDeviceReady) for SX126xCheckDeviceReady
    sx126x-board.o(i.SX126xWriteCommand) refers to memcpya.o(.text) for __aeabi_memcpy
    sx126x-board.o(i.SX126xWriteCommand) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xWriteCommand) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit) for HAL_SPI_Transmit
    sx126x-board.o(i.SX126xWriteCommand) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x-board.o(i.SX126xWriteCommand) refers to sx126x-board.o(.bss) for .bss
    sx126x-board.o(i.SX126xWriteCommand) refers to main.o(.bss) for hspi1
    sx126x-board.o(i.SX126xWriteRegister) refers to sx126x-board.o(i.SX126xWriteRegisters) for SX126xWriteRegisters
    sx126x-board.o(i.SX126xWriteRegisters) refers to sx126x.o(i.SX126xCheckDeviceReady) for SX126xCheckDeviceReady
    sx126x-board.o(i.SX126xWriteRegisters) refers to memcpya.o(.text) for __aeabi_memcpy
    sx126x-board.o(i.SX126xWriteRegisters) refers to stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    sx126x-board.o(i.SX126xWriteRegisters) refers to stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit) for HAL_SPI_Transmit
    sx126x-board.o(i.SX126xWriteRegisters) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x-board.o(i.SX126xWriteRegisters) refers to sx126x-board.o(.bss) for .bss
    sx126x-board.o(i.SX126xWriteRegisters) refers to main.o(.bss) for hspi1
    timer.o(i.DelayMs) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    timer.o(i.TimerGetCurrentTime) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    timer.o(i.TimerGetElapsedTime) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    timer.o(i.TimerInit) refers to timer.o(.bss) for .bss
    timer.o(i.TimerService) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    timer.o(i.TimerService) refers to timer.o(.data) for .data
    timer.o(i.TimerService) refers to timer.o(.bss) for .bss
    timer.o(i.TimerStart) refers to stm32f1xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    radio.o(i.RadioAddRegisterToRetentionList) refers to sx126x-board.o(i.SX126xReadRegisters) for SX126xReadRegisters
    radio.o(i.RadioAddRegisterToRetentionList) refers to sx126x-board.o(i.SX126xWriteRegisters) for SX126xWriteRegisters
    radio.o(i.RadioGetFskBandwidthRegValue) refers to radio.o(.constdata) for .constdata
    radio.o(i.RadioGetStatus) refers to sx126x-board.o(i.SX126xGetOperatingMode) for SX126xGetOperatingMode
    radio.o(i.RadioGetWakeupTime) refers to sx126x-board.o(i.SX126xGetBoardTcxoWakeupTime) for SX126xGetBoardTcxoWakeupTime
    radio.o(i.RadioInit) refers to sx126x.o(i.SX126xInit) for SX126xInit
    radio.o(i.RadioInit) refers to sx126x.o(i.SX126xSetStandby) for SX126xSetStandby
    radio.o(i.RadioInit) refers to sx126x.o(i.SX126xSetRegulatorMode) for SX126xSetRegulatorMode
    radio.o(i.RadioInit) refers to sx126x.o(i.SX126xSetBufferBaseAddress) for SX126xSetBufferBaseAddress
    radio.o(i.RadioInit) refers to sx126x.o(i.SX126xSetTxParams) for SX126xSetTxParams
    radio.o(i.RadioInit) refers to sx126x.o(i.SX126xSetDioIrqParams) for SX126xSetDioIrqParams
    radio.o(i.RadioInit) refers to radio.o(i.RadioAddRegisterToRetentionList) for RadioAddRegisterToRetentionList
    radio.o(i.RadioInit) refers to timer.o(i.TimerInit) for TimerInit
    radio.o(i.RadioInit) refers to radio.o(.data) for .data
    radio.o(i.RadioInit) refers to radio.o(i.RadioOnDioIrq) for RadioOnDioIrq
    radio.o(i.RadioInit) refers to radio.o(i.RadioOnTxTimeoutIrq) for RadioOnTxTimeoutIrq
    radio.o(i.RadioInit) refers to radio.o(.bss) for .bss
    radio.o(i.RadioInit) refers to radio.o(i.RadioOnRxTimeoutIrq) for RadioOnRxTimeoutIrq
    radio.o(i.RadioIrqProcess) refers to sx126x.o(i.SX126xGetIrqStatus) for SX126xGetIrqStatus
    radio.o(i.RadioIrqProcess) refers to sx126x.o(i.SX126xClearIrqStatus) for SX126xClearIrqStatus
    radio.o(i.RadioIrqProcess) refers to sx126x-board.o(i.SX126xGetDio1PinState) for SX126xGetDio1PinState
    radio.o(i.RadioIrqProcess) refers to timer.o(i.TimerStop) for TimerStop
    radio.o(i.RadioIrqProcess) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    radio.o(i.RadioIrqProcess) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    radio.o(i.RadioIrqProcess) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    radio.o(i.RadioIrqProcess) refers to sx126x.o(i.SX126xGetPayload) for SX126xGetPayload
    radio.o(i.RadioIrqProcess) refers to sx126x.o(i.SX126xGetPacketStatus) for SX126xGetPacketStatus
    radio.o(i.RadioIrqProcess) refers to sx126x-board.o(i.SX126xGetOperatingMode) for SX126xGetOperatingMode
    radio.o(i.RadioIrqProcess) refers to radio.o(.data) for .data
    radio.o(i.RadioIrqProcess) refers to radio.o(.bss) for .bss
    radio.o(i.RadioIsChannelFree) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioIsChannelFree) refers to sx126x.o(i.SX126xSetRfFrequency) for SX126xSetRfFrequency
    radio.o(i.RadioIsChannelFree) refers to radio.o(i.RadioSetRxConfig) for RadioSetRxConfig
    radio.o(i.RadioIsChannelFree) refers to radio.o(i.RadioRx) for RadioRx
    radio.o(i.RadioIsChannelFree) refers to timer.o(i.DelayMs) for DelayMs
    radio.o(i.RadioIsChannelFree) refers to timer.o(i.TimerGetCurrentTime) for TimerGetCurrentTime
    radio.o(i.RadioIsChannelFree) refers to sx126x.o(i.SX126xGetRssiInst) for SX126xGetRssiInst
    radio.o(i.RadioIsChannelFree) refers to timer.o(i.TimerGetElapsedTime) for TimerGetElapsedTime
    radio.o(i.RadioIsChannelFree) refers to radio.o(i.RadioSleep) for RadioSleep
    radio.o(i.RadioOnDioIrq) refers to radio.o(.data) for .data
    radio.o(i.RadioOnRxTimeoutIrq) refers to radio.o(.data) for .data
    radio.o(i.RadioOnTxTimeoutIrq) refers to radio.o(.data) for .data
    radio.o(i.RadioRandom) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioRandom) refers to sx126x.o(i.SX126xSetDioIrqParams) for SX126xSetDioIrqParams
    radio.o(i.RadioRandom) refers to sx126x.o(i.SX126xGetRandom) for SX126xGetRandom
    radio.o(i.RadioRead) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    radio.o(i.RadioReadBuffer) refers to sx126x-board.o(i.SX126xReadRegisters) for SX126xReadRegisters
    radio.o(i.RadioRssi) refers to sx126x.o(i.SX126xGetRssiInst) for SX126xGetRssiInst
    radio.o(i.RadioRx) refers to sx126x.o(i.SX126xSetDioIrqParams) for SX126xSetDioIrqParams
    radio.o(i.RadioRx) refers to timer.o(i.TimerSetValue) for TimerSetValue
    radio.o(i.RadioRx) refers to timer.o(i.TimerStart) for TimerStart
    radio.o(i.RadioRx) refers to sx126x.o(i.SX126xSetRx) for SX126xSetRx
    radio.o(i.RadioRx) refers to radio.o(.bss) for .bss
    radio.o(i.RadioRx) refers to radio.o(.data) for .data
    radio.o(i.RadioRxBoosted) refers to sx126x.o(i.SX126xSetDioIrqParams) for SX126xSetDioIrqParams
    radio.o(i.RadioRxBoosted) refers to timer.o(i.TimerSetValue) for TimerSetValue
    radio.o(i.RadioRxBoosted) refers to timer.o(i.TimerStart) for TimerStart
    radio.o(i.RadioRxBoosted) refers to sx126x.o(i.SX126xSetRxBoosted) for SX126xSetRxBoosted
    radio.o(i.RadioRxBoosted) refers to radio.o(.bss) for .bss
    radio.o(i.RadioRxBoosted) refers to radio.o(.data) for .data
    radio.o(i.RadioSend) refers to sx126x.o(i.SX126xSetDioIrqParams) for SX126xSetDioIrqParams
    radio.o(i.RadioSend) refers to sx126x.o(i.SX126xGetPacketType) for SX126xGetPacketType
    radio.o(i.RadioSend) refers to sx126x.o(i.SX126xSetPacketParams) for SX126xSetPacketParams
    radio.o(i.RadioSend) refers to sx126x.o(i.SX126xSendPayload) for SX126xSendPayload
    radio.o(i.RadioSend) refers to timer.o(i.TimerSetValue) for TimerSetValue
    radio.o(i.RadioSend) refers to timer.o(i.TimerStart) for TimerStart
    radio.o(i.RadioSend) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSend) refers to radio.o(.data) for .data
    radio.o(i.RadioSetChannel) refers to sx126x.o(i.SX126xSetRfFrequency) for SX126xSetRfFrequency
    radio.o(i.RadioSetMaxPayloadLength) refers to sx126x.o(i.SX126xSetPacketParams) for SX126xSetPacketParams
    radio.o(i.RadioSetMaxPayloadLength) refers to radio.o(.data) for .data
    radio.o(i.RadioSetMaxPayloadLength) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetModem) refers to sx126x.o(i.SX126xSetPacketType) for SX126xSetPacketType
    radio.o(i.RadioSetModem) refers to radio.o(i.RadioSetPublicNetwork) for RadioSetPublicNetwork
    radio.o(i.RadioSetModem) refers to radio.o(.data) for .data
    radio.o(i.RadioSetPublicNetwork) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetPublicNetwork) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    radio.o(i.RadioSetPublicNetwork) refers to radio.o(.data) for .data
    radio.o(i.RadioSetRxConfig) refers to sx126x.o(i.SX126xSetStopRxTimerOnPreambleDetect) for SX126xSetStopRxTimerOnPreambleDetect
    radio.o(i.RadioSetRxConfig) refers to radio.o(i.RadioGetFskBandwidthRegValue) for RadioGetFskBandwidthRegValue
    radio.o(i.RadioSetRxConfig) refers to sx126x.o(i.SX126xSetStandby) for SX126xSetStandby
    radio.o(i.RadioSetRxConfig) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetRxConfig) refers to sx126x.o(i.SX126xSetModulationParams) for SX126xSetModulationParams
    radio.o(i.RadioSetRxConfig) refers to sx126x.o(i.SX126xSetPacketParams) for SX126xSetPacketParams
    radio.o(i.RadioSetRxConfig) refers to sx126x.o(i.SX126xSetSyncWord) for SX126xSetSyncWord
    radio.o(i.RadioSetRxConfig) refers to sx126x.o(i.SX126xSetWhiteningSeed) for SX126xSetWhiteningSeed
    radio.o(i.RadioSetRxConfig) refers to sx126x.o(i.SX126xSetLoRaSymbNumTimeout) for SX126xSetLoRaSymbNumTimeout
    radio.o(i.RadioSetRxConfig) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    radio.o(i.RadioSetRxConfig) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    radio.o(i.RadioSetRxConfig) refers to radio.o(.data) for .data
    radio.o(i.RadioSetRxConfig) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetRxConfig) refers to radio.o(.constdata) for .constdata
    radio.o(i.RadioSetRxDutyCycle) refers to sx126x.o(i.SX126xSetRxDutyCycle) for SX126xSetRxDutyCycle
    radio.o(i.RadioSetTxConfig) refers to radio.o(i.RadioGetFskBandwidthRegValue) for RadioGetFskBandwidthRegValue
    radio.o(i.RadioSetTxConfig) refers to sx126x.o(i.SX126xSetStandby) for SX126xSetStandby
    radio.o(i.RadioSetTxConfig) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(i.RadioSetTxConfig) refers to sx126x.o(i.SX126xSetModulationParams) for SX126xSetModulationParams
    radio.o(i.RadioSetTxConfig) refers to sx126x.o(i.SX126xSetPacketParams) for SX126xSetPacketParams
    radio.o(i.RadioSetTxConfig) refers to sx126x.o(i.SX126xSetSyncWord) for SX126xSetSyncWord
    radio.o(i.RadioSetTxConfig) refers to sx126x.o(i.SX126xSetWhiteningSeed) for SX126xSetWhiteningSeed
    radio.o(i.RadioSetTxConfig) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    radio.o(i.RadioSetTxConfig) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    radio.o(i.RadioSetTxConfig) refers to sx126x-board.o(i.SX126xSetRfTxPower) for SX126xSetRfTxPower
    radio.o(i.RadioSetTxConfig) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSetTxConfig) refers to radio.o(.constdata) for .constdata
    radio.o(i.RadioSetTxConfig) refers to radio.o(.data) for .data
    radio.o(i.RadioSetTxContinuousWave) refers to sx126x.o(i.SX126xSetRfFrequency) for SX126xSetRfFrequency
    radio.o(i.RadioSetTxContinuousWave) refers to sx126x-board.o(i.SX126xSetRfTxPower) for SX126xSetRfTxPower
    radio.o(i.RadioSetTxContinuousWave) refers to sx126x.o(i.SX126xSetTxContinuousWave) for SX126xSetTxContinuousWave
    radio.o(i.RadioSetTxContinuousWave) refers to timer.o(i.TimerSetValue) for TimerSetValue
    radio.o(i.RadioSetTxContinuousWave) refers to timer.o(i.TimerStart) for TimerStart
    radio.o(i.RadioSetTxContinuousWave) refers to radio.o(.bss) for .bss
    radio.o(i.RadioSleep) refers to sx126x.o(i.SX126xSetSleep) for SX126xSetSleep
    radio.o(i.RadioSleep) refers to timer.o(i.DelayMs) for DelayMs
    radio.o(i.RadioStandby) refers to sx126x.o(i.SX126xSetStandby) for SX126xSetStandby
    radio.o(i.RadioStartCad) refers to sx126x.o(i.SX126xSetDioIrqParams) for SX126xSetDioIrqParams
    radio.o(i.RadioStartCad) refers to sx126x.o(i.SX126xSetCad) for SX126xSetCad
    radio.o(i.RadioTimeOnAir) refers to radio.o(i.RadioGetLoRaTimeOnAirNumerator) for RadioGetLoRaTimeOnAirNumerator
    radio.o(i.RadioTimeOnAir) refers to radio.o(.constdata) for .constdata
    radio.o(i.RadioWrite) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    radio.o(i.RadioWriteBuffer) refers to sx126x-board.o(i.SX126xWriteRegisters) for SX126xWriteRegisters
    radio.o(.constdata) refers to radio.o(i.RadioInit) for RadioInit
    radio.o(.constdata) refers to radio.o(i.RadioGetStatus) for RadioGetStatus
    radio.o(.constdata) refers to radio.o(i.RadioSetModem) for RadioSetModem
    radio.o(.constdata) refers to radio.o(i.RadioSetChannel) for RadioSetChannel
    radio.o(.constdata) refers to radio.o(i.RadioIsChannelFree) for RadioIsChannelFree
    radio.o(.constdata) refers to radio.o(i.RadioRandom) for RadioRandom
    radio.o(.constdata) refers to radio.o(i.RadioSetRxConfig) for RadioSetRxConfig
    radio.o(.constdata) refers to radio.o(i.RadioSetTxConfig) for RadioSetTxConfig
    radio.o(.constdata) refers to radio.o(i.RadioCheckRfFrequency) for RadioCheckRfFrequency
    radio.o(.constdata) refers to radio.o(i.RadioTimeOnAir) for RadioTimeOnAir
    radio.o(.constdata) refers to radio.o(i.RadioSend) for RadioSend
    radio.o(.constdata) refers to radio.o(i.RadioSleep) for RadioSleep
    radio.o(.constdata) refers to radio.o(i.RadioStandby) for RadioStandby
    radio.o(.constdata) refers to radio.o(i.RadioRx) for RadioRx
    radio.o(.constdata) refers to radio.o(i.RadioStartCad) for RadioStartCad
    radio.o(.constdata) refers to radio.o(i.RadioSetTxContinuousWave) for RadioSetTxContinuousWave
    radio.o(.constdata) refers to radio.o(i.RadioRssi) for RadioRssi
    radio.o(.constdata) refers to radio.o(i.RadioWrite) for RadioWrite
    radio.o(.constdata) refers to radio.o(i.RadioRead) for RadioRead
    radio.o(.constdata) refers to radio.o(i.RadioWriteBuffer) for RadioWriteBuffer
    radio.o(.constdata) refers to radio.o(i.RadioReadBuffer) for RadioReadBuffer
    radio.o(.constdata) refers to radio.o(i.RadioSetMaxPayloadLength) for RadioSetMaxPayloadLength
    radio.o(.constdata) refers to radio.o(i.RadioSetPublicNetwork) for RadioSetPublicNetwork
    radio.o(.constdata) refers to radio.o(i.RadioGetWakeupTime) for RadioGetWakeupTime
    radio.o(.constdata) refers to radio.o(i.RadioIrqProcess) for RadioIrqProcess
    radio.o(.constdata) refers to radio.o(i.RadioRxBoosted) for RadioRxBoosted
    radio.o(.constdata) refers to radio.o(i.RadioSetRxDutyCycle) for RadioSetRxDutyCycle
    sx126x.o(i.SX126xCalibrate) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xCalibrateImage) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xCheckDeviceReady) refers to sx126x-board.o(i.SX126xGetOperatingMode) for SX126xGetOperatingMode
    sx126x.o(i.SX126xCheckDeviceReady) refers to sx126x-board.o(i.SX126xWakeup) for SX126xWakeup
    sx126x.o(i.SX126xCheckDeviceReady) refers to sx126x-board.o(i.SX126xAntSwOn) for SX126xAntSwOn
    sx126x.o(i.SX126xCheckDeviceReady) refers to sx126x-board.o(i.SX126xWaitOnBusy) for SX126xWaitOnBusy
    sx126x.o(i.SX126xClearDeviceErrors) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xClearIrqStatus) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xGetDeviceErrors) refers to sx126x-board.o(i.SX126xReadCommand) for SX126xReadCommand
    sx126x.o(i.SX126xGetIrqStatus) refers to sx126x-board.o(i.SX126xReadCommand) for SX126xReadCommand
    sx126x.o(i.SX126xGetPacketStatus) refers to sx126x-board.o(i.SX126xReadCommand) for SX126xReadCommand
    sx126x.o(i.SX126xGetPacketStatus) refers to memseta.o(.text) for __aeabi_memclr4
    sx126x.o(i.SX126xGetPacketStatus) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xGetPacketType) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xGetPayload) refers to sx126x.o(i.SX126xGetRxBufferStatus) for SX126xGetRxBufferStatus
    sx126x.o(i.SX126xGetPayload) refers to sx126x-board.o(i.SX126xReadBuffer) for SX126xReadBuffer
    sx126x.o(i.SX126xGetRandom) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    sx126x.o(i.SX126xGetRandom) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    sx126x.o(i.SX126xGetRandom) refers to sx126x.o(i.SX126xSetRx) for SX126xSetRx
    sx126x.o(i.SX126xGetRandom) refers to sx126x-board.o(i.SX126xReadRegisters) for SX126xReadRegisters
    sx126x.o(i.SX126xGetRandom) refers to sx126x.o(i.SX126xSetStandby) for SX126xSetStandby
    sx126x.o(i.SX126xGetRssiInst) refers to sx126x-board.o(i.SX126xReadCommand) for SX126xReadCommand
    sx126x.o(i.SX126xGetRxBufferStatus) refers to sx126x-board.o(i.SX126xReadCommand) for SX126xReadCommand
    sx126x.o(i.SX126xGetRxBufferStatus) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    sx126x.o(i.SX126xGetRxBufferStatus) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xGetStatus) refers to sx126x-board.o(i.SX126xReadCommand) for SX126xReadCommand
    sx126x.o(i.SX126xInit) refers to sx126x-board.o(i.SX126xIoInit) for SX126xIoInit
    sx126x.o(i.SX126xInit) refers to sx126x-board.o(i.SX126xReset) for SX126xReset
    sx126x.o(i.SX126xInit) refers to sx126x-board.o(i.SX126xIoIrqInit) for SX126xIoIrqInit
    sx126x.o(i.SX126xInit) refers to sx126x-board.o(i.SX126xWakeup) for SX126xWakeup
    sx126x.o(i.SX126xInit) refers to sx126x.o(i.SX126xSetStandby) for SX126xSetStandby
    sx126x.o(i.SX126xInit) refers to sx126x-board.o(i.SX126xIoTcxoInit) for SX126xIoTcxoInit
    sx126x.o(i.SX126xInit) refers to sx126x-board.o(i.SX126xIoRfSwitchInit) for SX126xIoRfSwitchInit
    sx126x.o(i.SX126xInit) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xInit) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSendPayload) refers to sx126x.o(i.SX126xSetPayload) for SX126xSetPayload
    sx126x.o(i.SX126xSendPayload) refers to sx126x.o(i.SX126xSetTx) for SX126xSetTx
    sx126x.o(i.SX126xSetBufferBaseAddress) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetCad) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetCad) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetCadParams) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetCadParams) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetCrcPolynomial) refers to sx126x-board.o(i.SX126xWriteRegisters) for SX126xWriteRegisters
    sx126x.o(i.SX126xSetCrcPolynomial) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSetCrcSeed) refers to sx126x-board.o(i.SX126xWriteRegisters) for SX126xWriteRegisters
    sx126x.o(i.SX126xSetCrcSeed) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSetDio2AsRfSwitchCtrl) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetDio3AsTcxoCtrl) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetDioIrqParams) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetFs) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetFs) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetLoRaSymbNumTimeout) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetLoRaSymbNumTimeout) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    sx126x.o(i.SX126xSetModulationParams) refers to sx126x.o(i.SX126xSetPacketType) for SX126xSetPacketType
    sx126x.o(i.SX126xSetModulationParams) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetModulationParams) refers to sx126x.o(i.SX126xConvertFreqInHzToPllStep) for SX126xConvertFreqInHzToPllStep
    sx126x.o(i.SX126xSetModulationParams) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSetPaConfig) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetPacketParams) refers to sx126x.o(i.SX126xSetPacketType) for SX126xSetPacketType
    sx126x.o(i.SX126xSetPacketParams) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetPacketParams) refers to sx126x.o(i.SX126xSetCrcSeed) for SX126xSetCrcSeed
    sx126x.o(i.SX126xSetPacketParams) refers to sx126x.o(i.SX126xSetCrcPolynomial) for SX126xSetCrcPolynomial
    sx126x.o(i.SX126xSetPacketParams) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSetPacketType) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetPacketType) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSetPayload) refers to sx126x-board.o(i.SX126xWriteBuffer) for SX126xWriteBuffer
    sx126x.o(i.SX126xSetRegulatorMode) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetRfFrequency) refers to sx126x.o(i.SX126xCalibrateImage) for SX126xCalibrateImage
    sx126x.o(i.SX126xSetRfFrequency) refers to sx126x.o(i.SX126xConvertFreqInHzToPllStep) for SX126xConvertFreqInHzToPllStep
    sx126x.o(i.SX126xSetRfFrequency) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetRfFrequency) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSetRx) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetRx) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    sx126x.o(i.SX126xSetRx) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetRxBoosted) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetRxBoosted) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    sx126x.o(i.SX126xSetRxBoosted) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetRxDutyCycle) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetRxDutyCycle) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetRxTxFallbackMode) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetSleep) refers to sx126x-board.o(i.SX126xAntSwOff) for SX126xAntSwOff
    sx126x.o(i.SX126xSetSleep) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetSleep) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetSleep) refers to sx126x.o(.data) for .data
    sx126x.o(i.SX126xSetStandby) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetStandby) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetStopRxTimerOnPreambleDetect) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetSyncWord) refers to sx126x-board.o(i.SX126xWriteRegisters) for SX126xWriteRegisters
    sx126x.o(i.SX126xSetTx) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetTx) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetTxContinuousWave) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetTxContinuousWave) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetTxInfinitePreamble) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetTxInfinitePreamble) refers to sx126x-board.o(i.SX126xSetOperatingMode) for SX126xSetOperatingMode
    sx126x.o(i.SX126xSetTxParams) refers to sx126x-board.o(i.SX126xGetDeviceId) for SX126xGetDeviceId
    sx126x.o(i.SX126xSetTxParams) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    sx126x.o(i.SX126xSetTxParams) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    sx126x.o(i.SX126xSetTxParams) refers to sx126x.o(i.SX126xSetPaConfig) for SX126xSetPaConfig
    sx126x.o(i.SX126xSetTxParams) refers to sx126x-board.o(i.SX126xWriteCommand) for SX126xWriteCommand
    sx126x.o(i.SX126xSetWhiteningSeed) refers to sx126x-board.o(i.SX126xReadRegister) for SX126xReadRegister
    sx126x.o(i.SX126xSetWhiteningSeed) refers to sx126x-board.o(i.SX126xWriteRegister) for SX126xWriteRegister
    sx126x.o(i.SX126xSetWhiteningSeed) refers to sx126x.o(.data) for .data
    test.o(i.LoRa_Init) refers to printf8.o(i.__0printf$8) for __2printf
    test.o(i.LoRa_Init) refers to timer.o(i.DelayMs) for DelayMs
    test.o(i.LoRa_Init) refers to test.o(i.OnTxDone) for OnTxDone
    test.o(i.LoRa_Init) refers to test.o(.bss) for .bss
    test.o(i.LoRa_Init) refers to test.o(i.OnRxDone) for OnRxDone
    test.o(i.LoRa_Init) refers to test.o(i.OnTxTimeout) for OnTxTimeout
    test.o(i.LoRa_Init) refers to test.o(i.OnRxTimeout) for OnRxTimeout
    test.o(i.LoRa_Init) refers to test.o(i.OnRxError) for OnRxError
    test.o(i.LoRa_Init) refers to radio.o(.constdata) for Radio
    test.o(i.LoRa_Test_Handle) refers to printf8.o(i.__0printf$8) for __2printf
    test.o(i.LoRa_Test_Handle) refers to timer.o(i.TimerStart) for TimerStart
    test.o(i.LoRa_Test_Handle) refers to test.o(.data) for .data
    test.o(i.LoRa_Test_Handle) refers to test.o(.bss) for .bss
    test.o(i.LoRa_Test_Handle) refers to radio.o(.constdata) for Radio
    test.o(i.LoRa_Test_Main) refers to timer.o(i.TimerInit) for TimerInit
    test.o(i.LoRa_Test_Main) refers to timer.o(i.TimerSetValue) for TimerSetValue
    test.o(i.LoRa_Test_Main) refers to timer.o(i.TimerStart) for TimerStart
    test.o(i.LoRa_Test_Main) refers to timer.o(i.TimerService) for TimerService
    test.o(i.LoRa_Test_Main) refers to test.o(i.LoRa_Test_Handle) for LoRa_Test_Handle
    test.o(i.LoRa_Test_Main) refers to test.o(.bss) for .bss
    test.o(i.LoRa_Test_Main) refers to radio.o(.constdata) for Radio
    test.o(i.OnRxDone) refers to memcpya.o(.text) for __aeabi_memcpy
    test.o(i.OnRxDone) refers to printf8.o(i.__0printf$8) for __2printf
    test.o(i.OnRxDone) refers to test.o(.bss) for .bss
    test.o(i.OnRxError) refers to printf8.o(i.__0printf$8) for __2printf
    test.o(i.OnRxError) refers to radio.o(.constdata) for Radio
    test.o(i.OnRxTimeout) refers to printf8.o(i.__0printf$8) for __2printf
    test.o(i.OnRxTimeout) refers to radio.o(.constdata) for Radio
    test.o(i.OnTxDone) refers to printf8.o(i.__0printf$8) for __2printf
    test.o(i.OnTxDone) refers to radio.o(.constdata) for Radio
    test.o(i.OnTxTimeout) refers to printf8.o(i.__0printf$8) for __2printf
    test.o(i.OnTxTimeout) refers to radio.o(.constdata) for Radio
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to main.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to main.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to main.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to main.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to main.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to main.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to main.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to main.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to main.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to main.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to main.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to main.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to main.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to main.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to main.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to main.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to main.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to main.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to main.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to main.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to main.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to main.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to main.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to main.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to main.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to main.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to main.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to main.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to main.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to main.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to main.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to main.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to main.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to main.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to main.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to main.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to main.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to main.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to main.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to main.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to main.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to main.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to main.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to main.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_stm32f103xe.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_stm32f103xe.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr


==============================================================================

Removing Unused input sections from the image.

    Removing startup_stm32f103xe.o(HEAP), (512 bytes).
    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing main.o(.rrx_text), (6 bytes).
    Removing main.o(i.Error_Handler), (4 bytes).
    Removing stm32f1xx_it.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_it.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_it.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_msp.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_msp.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_msp.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_msp.o(i.HAL_SPI_MspDeInit), (40 bytes).
    Removing stm32f1xx_hal_msp.o(i.HAL_UART_MspDeInit), (44 bytes).
    Removing stm32f1xx_hal_gpio_ex.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_gpio_ex.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_gpio_ex.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_gpio_ex.o(i.HAL_GPIOEx_ConfigEventout), (20 bytes).
    Removing stm32f1xx_hal_gpio_ex.o(i.HAL_GPIOEx_DisableEventout), (16 bytes).
    Removing stm32f1xx_hal_gpio_ex.o(i.HAL_GPIOEx_EnableEventout), (16 bytes).
    Removing stm32f1xx_hal_spi.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_spi.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_spi.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_Abort), (288 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_Abort_IT), (288 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_DMAPause), (38 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_DMAResume), (38 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_DMAStop), (66 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_DeInit), (46 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_GetError), (4 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_GetState), (6 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_IRQHandler), (224 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_MspDeInit), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_MspInit), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_Receive), (346 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_DMA), (244 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_Receive_IT), (176 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_RxCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_RxHalfCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA), (292 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT), (164 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA), (216 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_IT), (148 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_TxCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_TxHalfCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_TxRxCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.HAL_SPI_TxRxHalfCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_2linesRxISR_16BIT), (48 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_2linesRxISR_8BIT), (48 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_2linesTxISR_16BIT), (48 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_2linesTxISR_8BIT), (48 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_AbortRx_ISR), (88 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_AbortTx_ISR), (28 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_CloseRxTx_ISR), (144 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_CloseRx_ISR), (76 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_CloseTx_ISR), (124 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMAAbortOnError), (16 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMAError), (34 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt), (10 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt), (10 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt), (10 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt), (106 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMARxAbortCallback), (98 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt), (100 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt), (90 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_DMATxAbortCallback), (112 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_EndRxTransaction), (92 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_RxISR_16BIT), (32 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_RxISR_8BIT), (32 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_TxISR_16BIT), (32 bytes).
    Removing stm32f1xx_hal_spi.o(i.SPI_TxISR_8BIT), (32 bytes).
    Removing stm32f1xx_hal.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal.o(i.HAL_DBGMCU_DisableDBGSleepMode), (16 bytes).
    Removing stm32f1xx_hal.o(i.HAL_DBGMCU_DisableDBGStandbyMode), (16 bytes).
    Removing stm32f1xx_hal.o(i.HAL_DBGMCU_DisableDBGStopMode), (16 bytes).
    Removing stm32f1xx_hal.o(i.HAL_DBGMCU_EnableDBGSleepMode), (16 bytes).
    Removing stm32f1xx_hal.o(i.HAL_DBGMCU_EnableDBGStandbyMode), (16 bytes).
    Removing stm32f1xx_hal.o(i.HAL_DBGMCU_EnableDBGStopMode), (16 bytes).
    Removing stm32f1xx_hal.o(i.HAL_DeInit), (32 bytes).
    Removing stm32f1xx_hal.o(i.HAL_Delay), (36 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetDEVID), (16 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetHalVersion), (8 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetREVID), (12 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetTickFreq), (12 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetTickPrio), (12 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetUIDw0), (12 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetUIDw1), (12 bytes).
    Removing stm32f1xx_hal.o(i.HAL_GetUIDw2), (12 bytes).
    Removing stm32f1xx_hal.o(i.HAL_MspDeInit), (2 bytes).
    Removing stm32f1xx_hal.o(i.HAL_MspInit), (2 bytes).
    Removing stm32f1xx_hal.o(i.HAL_ResumeTick), (14 bytes).
    Removing stm32f1xx_hal.o(i.HAL_SetTickFreq), (36 bytes).
    Removing stm32f1xx_hal.o(i.HAL_SuspendTick), (14 bytes).
    Removing stm32f1xx_hal_rcc.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_rcc.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_rcc.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_CSSCallback), (2 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_DeInit), (220 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_DisableCSS), (12 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_EnableCSS), (12 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_GetClockConfig), (64 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq), (12 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_GetOscConfig), (144 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_MCOConfig), (72 bytes).
    Removing stm32f1xx_hal_rcc.o(i.HAL_RCC_NMI_IRQHandler), (24 bytes).
    Removing stm32f1xx_hal_rcc_ex.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_rcc_ex.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_rcc_ex.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKConfig), (52 bytes).
    Removing stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq), (212 bytes).
    Removing stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig), (236 bytes).
    Removing stm32f1xx_hal_gpio.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_gpio.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_gpio.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_gpio.o(i.HAL_GPIO_DeInit), (288 bytes).
    Removing stm32f1xx_hal_gpio.o(i.HAL_GPIO_EXTI_Callback), (2 bytes).
    Removing stm32f1xx_hal_gpio.o(i.HAL_GPIO_LockPin), (34 bytes).
    Removing stm32f1xx_hal_gpio.o(i.HAL_GPIO_TogglePin), (16 bytes).
    Removing stm32f1xx_hal_dma.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_dma.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_dma.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_dma.o(i.DMA_SetConfig), (42 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_Abort), (70 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT), (304 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_DeInit), (128 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_GetError), (4 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_GetState), (6 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_IRQHandler), (584 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_Init), (124 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_PollForTransfer), (988 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_RegisterCallback), (74 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_Start), (80 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT), (112 bytes).
    Removing stm32f1xx_hal_dma.o(i.HAL_DMA_UnRegisterCallback), (82 bytes).
    Removing stm32f1xx_hal_cortex.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_cortex.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_cortex.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_NVIC_ClearPendingIRQ), (26 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_NVIC_GetActive), (36 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_NVIC_GetPendingIRQ), (36 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_NVIC_GetPriority), (82 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_NVIC_GetPriorityGrouping), (16 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPendingIRQ), (26 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_NVIC_SystemReset), (36 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig), (24 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Callback), (2 bytes).
    Removing stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler), (8 bytes).
    Removing stm32f1xx_hal_pwr.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_pwr.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_pwr.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_ConfigPVD), (124 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_DeInit), (24 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_DisableBkUpAccess), (12 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_DisablePVD), (12 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_DisableSEVOnPend), (16 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_DisableSleepOnExit), (16 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_DisableWakeUpPin), (28 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess), (12 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnablePVD), (12 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnableSEVOnPend), (16 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnableSleepOnExit), (16 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnableWakeUpPin), (28 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnterSLEEPMode), (32 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnterSTANDBYMode), (32 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_EnterSTOPMode), (68 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_PVDCallback), (2 bytes).
    Removing stm32f1xx_hal_pwr.o(i.HAL_PWR_PVD_IRQHandler), (28 bytes).
    Removing stm32f1xx_hal_pwr.o(i.PWR_OverloadWfe), (6 bytes).
    Removing stm32f1xx_hal_flash.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_flash.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_flash.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_flash.o(i.FLASH_Program_HalfWord), (28 bytes).
    Removing stm32f1xx_hal_flash.o(i.FLASH_SetErrorCode), (92 bytes).
    Removing stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation), (84 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_EndOfOperationCallback), (2 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_GetError), (12 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler), (264 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_Lock), (20 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_OB_Launch), (4 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_OB_Lock), (20 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_OB_Unlock), (36 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_OperationErrorCallback), (2 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_Program), (128 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_Program_IT), (100 bytes).
    Removing stm32f1xx_hal_flash.o(i.HAL_FLASH_Unlock), (40 bytes).
    Removing stm32f1xx_hal_flash.o(.bss), (32 bytes).
    Removing stm32f1xx_hal_flash_ex.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_flash_ex.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_flash_ex.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.FLASH_MassErase), (36 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP), (176 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP), (176 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.FLASH_OB_GetRDP), (24 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig), (100 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.FLASH_PageErase), (36 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase), (168 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT), (84 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBErase), (84 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig), (36 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetUserData), (32 bytes).
    Removing stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram), (200 bytes).
    Removing stm32f1xx_hal_exti.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_exti.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_exti.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_ClearConfigLine), (104 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_ClearPending), (20 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_GenerateSWI), (20 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_GetConfigLine), (144 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_GetHandle), (12 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_GetPending), (24 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_IRQHandler), (36 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_RegisterCallback), (14 bytes).
    Removing stm32f1xx_hal_exti.o(i.HAL_EXTI_SetConfigLine), (164 bytes).
    Removing stm32f1xx_hal_tim.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_tim.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_tim.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_tim_ex.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_tim_ex.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_tim_ex.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_uart.o(.rev16_text), (4 bytes).
    Removing stm32f1xx_hal_uart.o(.revsh_text), (4 bytes).
    Removing stm32f1xx_hal_uart.o(.rrx_text), (6 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_HalfDuplex_EnableReceiver), (50 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_HalfDuplex_EnableTransmitter), (50 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_HalfDuplex_Init), (108 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_LIN_Init), (128 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_LIN_SendBreak), (46 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_MultiProcessor_EnterMuteMode), (46 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_MultiProcessor_ExitMuteMode), (46 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_MultiProcessor_Init), (142 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UARTEx_ReceiveToIdle), (254 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UARTEx_ReceiveToIdle_DMA), (74 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UARTEx_ReceiveToIdle_IT), (74 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_Abort), (156 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_AbortCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceive), (106 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceiveCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_AbortReceive_IT), (112 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmit), (78 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmitCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_AbortTransmit_IT), (84 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_Abort_IT), (188 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_DMAPause), (102 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_DMAResume), (94 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_DMAStop), (88 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_DeInit), (52 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_GetError), (4 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_GetState), (10 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler), (524 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_MspDeInit), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_MspInit), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_Receive), (192 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_Receive_DMA), (42 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_Receive_IT), (42 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_RxCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_RxHalfCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_Transmit_DMA), (128 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_Transmit_IT), (62 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_TxCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback), (2 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError), (16 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMAError), (74 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMAReceiveCplt), (90 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMARxAbortCallback), (44 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMARxHalfCplt), (26 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMARxOnlyAbortCallback), (22 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMATransmitCplt), (46 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMATxAbortCallback), (44 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMATxHalfCplt), (10 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_DMATxOnlyAbortCallback), (20 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_EndRxTransfer), (48 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_EndTxTransfer), (18 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_Receive_IT), (182 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA), (112 bytes).
    Removing stm32f1xx_hal_uart.o(i.UART_Start_Receive_IT), (54 bytes).
    Removing system_stm32f1xx.o(.rev16_text), (4 bytes).
    Removing system_stm32f1xx.o(.revsh_text), (4 bytes).
    Removing system_stm32f1xx.o(.rrx_text), (6 bytes).
    Removing system_stm32f1xx.o(i.SystemCoreClockUpdate), (104 bytes).
    Removing sx126x-board.o(.rev16_text), (4 bytes).
    Removing sx126x-board.o(.revsh_text), (4 bytes).
    Removing sx126x-board.o(.rrx_text), (6 bytes).
    Removing sx126x-board.o(i.SX126xAntSwRx), (2 bytes).
    Removing sx126x-board.o(i.SX126xAntSwTx), (2 bytes).
    Removing sx126x-board.o(i.SX126xCheckRfFrequency), (4 bytes).
    Removing sx126x-board.o(i.SX126xIoDbgInit), (80 bytes).
    Removing sx126x-board.o(i.SX126xIoDeInit), (2 bytes).
    Removing timer.o(.rev16_text), (4 bytes).
    Removing timer.o(.revsh_text), (4 bytes).
    Removing timer.o(.rrx_text), (6 bytes).
    Removing radio.o(.rev16_text), (4 bytes).
    Removing radio.o(.revsh_text), (4 bytes).
    Removing radio.o(.rrx_text), (6 bytes).
    Removing sx126x.o(.rev16_text), (4 bytes).
    Removing sx126x.o(.revsh_text), (4 bytes).
    Removing sx126x.o(.rrx_text), (6 bytes).
    Removing sx126x.o(i.SX126xCalibrate), (70 bytes).
    Removing sx126x.o(i.SX126xClearDeviceErrors), (18 bytes).
    Removing sx126x.o(i.SX126xGetDeviceErrors), (88 bytes).
    Removing sx126x.o(i.SX126xGetStatus), (32 bytes).
    Removing sx126x.o(i.SX126xSetCadParams), (54 bytes).
    Removing sx126x.o(i.SX126xSetDio3AsTcxoCtrl), (38 bytes).
    Removing sx126x.o(i.SX126xSetFs), (22 bytes).
    Removing sx126x.o(i.SX126xSetRxTxFallbackMode), (14 bytes).
    Removing sx126x.o(i.SX126xSetTxInfinitePreamble), (22 bytes).
    Removing test.o(.rev16_text), (4 bytes).
    Removing test.o(.revsh_text), (4 bytes).
    Removing test.o(.rrx_text), (6 bytes).
    Removing dadd.o(.text), (334 bytes).
    Removing dmul.o(.text), (228 bytes).
    Removing ddiv.o(.text), (222 bytes).
    Removing dfixul.o(.text), (48 bytes).
    Removing cdrcmple.o(.text), (48 bytes).
    Removing depilogue.o(.text), (186 bytes).

319 unused section(s) (total 18236 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal.c 0x00000000   Number         0  stm32f1xx_hal.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_cortex.c 0x00000000   Number         0  stm32f1xx_hal_cortex.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_dma.c 0x00000000   Number         0  stm32f1xx_hal_dma.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_exti.c 0x00000000   Number         0  stm32f1xx_hal_exti.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_flash.c 0x00000000   Number         0  stm32f1xx_hal_flash.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_flash_ex.c 0x00000000   Number         0  stm32f1xx_hal_flash_ex.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_gpio.c 0x00000000   Number         0  stm32f1xx_hal_gpio.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_gpio_ex.c 0x00000000   Number         0  stm32f1xx_hal_gpio_ex.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_pwr.c 0x00000000   Number         0  stm32f1xx_hal_pwr.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_rcc.c 0x00000000   Number         0  stm32f1xx_hal_rcc.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_rcc_ex.c 0x00000000   Number         0  stm32f1xx_hal_rcc_ex.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_spi.c 0x00000000   Number         0  stm32f1xx_hal_spi.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_tim.c 0x00000000   Number         0  stm32f1xx_hal_tim.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_tim_ex.c 0x00000000   Number         0  stm32f1xx_hal_tim_ex.o ABSOLUTE
    ../Drivers/STM32F1xx_HAL_Driver/Src/stm32f1xx_hal_uart.c 0x00000000   Number         0  stm32f1xx_hal_uart.o ABSOLUTE
    ../Src/main.c                            0x00000000   Number         0  main.o ABSOLUTE
    ../Src/stm32f1xx_hal_msp.c               0x00000000   Number         0  stm32f1xx_hal_msp.o ABSOLUTE
    ../Src/stm32f1xx_it.c                    0x00000000   Number         0  stm32f1xx_it.o ABSOLUTE
    ../Src/system_stm32f1xx.c                0x00000000   Number         0  system_stm32f1xx.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal.c 0x00000000   Number         0  stm32f1xx_hal.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_cortex.c 0x00000000   Number         0  stm32f1xx_hal_cortex.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_dma.c 0x00000000   Number         0  stm32f1xx_hal_dma.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_exti.c 0x00000000   Number         0  stm32f1xx_hal_exti.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_flash.c 0x00000000   Number         0  stm32f1xx_hal_flash.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_flash_ex.c 0x00000000   Number         0  stm32f1xx_hal_flash_ex.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_gpio.c 0x00000000   Number         0  stm32f1xx_hal_gpio.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_gpio_ex.c 0x00000000   Number         0  stm32f1xx_hal_gpio_ex.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_pwr.c 0x00000000   Number         0  stm32f1xx_hal_pwr.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_rcc.c 0x00000000   Number         0  stm32f1xx_hal_rcc.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_rcc_ex.c 0x00000000   Number         0  stm32f1xx_hal_rcc_ex.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_spi.c 0x00000000   Number         0  stm32f1xx_hal_spi.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_tim.c 0x00000000   Number         0  stm32f1xx_hal_tim.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_tim_ex.c 0x00000000   Number         0  stm32f1xx_hal_tim_ex.o ABSOLUTE
    ..\Drivers\STM32F1xx_HAL_Driver\Src\stm32f1xx_hal_uart.c 0x00000000   Number         0  stm32f1xx_hal_uart.o ABSOLUTE
    ..\Src\main.c                            0x00000000   Number         0  main.o ABSOLUTE
    ..\Src\stm32f1xx_hal_msp.c               0x00000000   Number         0  stm32f1xx_hal_msp.o ABSOLUTE
    ..\Src\stm32f1xx_it.c                    0x00000000   Number         0  stm32f1xx_it.o ABSOLUTE
    ..\Src\system_stm32f1xx.c                0x00000000   Number         0  system_stm32f1xx.o ABSOLUTE
    ..\WH-LR30-H10\Board\sx126x-board.c      0x00000000   Number         0  sx126x-board.o ABSOLUTE
    ..\WH-LR30-H10\Board\timer.c             0x00000000   Number         0  timer.o ABSOLUTE
    ..\WH-LR30-H10\Radio\sx126x\radio.c      0x00000000   Number         0  radio.o ABSOLUTE
    ..\WH-LR30-H10\Radio\sx126x\sx126x.c     0x00000000   Number         0  sx126x.o ABSOLUTE
    ..\WH-LR30-H10\Test\test.c               0x00000000   Number         0  test.o ABSOLUTE
    ..\\WH-LR30-H10\\Board\\sx126x-board.c   0x00000000   Number         0  sx126x-board.o ABSOLUTE
    ..\\WH-LR30-H10\\Board\\timer.c          0x00000000   Number         0  timer.o ABSOLUTE
    ..\\WH-LR30-H10\\Radio\\sx126x\\radio.c  0x00000000   Number         0  radio.o ABSOLUTE
    ..\\WH-LR30-H10\\Radio\\sx126x\\sx126x.c 0x00000000   Number         0  sx126x.o ABSOLUTE
    ..\\WH-LR30-H10\\Test\\test.c            0x00000000   Number         0  test.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    startup_stm32f103xe.s                    0x00000000   Number         0  startup_stm32f103xe.o ABSOLUTE
    RESET                                    0x08000000   Section      304  startup_stm32f103xe.o(RESET)
    .ARM.Collect$$$$00000000                 0x08000130   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x08000130   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x08000134   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x08000138   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x08000138   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x08000138   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x08000140   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x08000140   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x08000140   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x08000140   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x08000144   Section       36  startup_stm32f103xe.o(.text)
    .text                                    0x08000168   Section        0  llushr.o(.text)
    .text                                    0x08000188   Section        0  memcpya.o(.text)
    .text                                    0x080001ac   Section        0  memseta.o(.text)
    .text                                    0x080001d0   Section        0  uldiv.o(.text)
    .text                                    0x08000234   Section       36  init.o(.text)
    .text                                    0x08000258   Section        0  llshl.o(.text)
    i.BusFault_Handler                       0x08000276   Section        0  stm32f1xx_it.o(i.BusFault_Handler)
    i.DebugMon_Handler                       0x08000278   Section        0  stm32f1xx_it.o(i.DebugMon_Handler)
    i.DelayMs                                0x0800027c   Section        0  timer.o(i.DelayMs)
    i.EXTI0_IRQHandler                       0x08000294   Section        0  stm32f1xx_it.o(i.EXTI0_IRQHandler)
    i.HAL_GPIO_EXTI_Callback                 0x0800029c   Section        0  sx126x-board.o(i.HAL_GPIO_EXTI_Callback)
    i.HAL_GPIO_EXTI_IRQHandler               0x080002b8   Section        0  stm32f1xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler)
    i.HAL_GPIO_Init                          0x080002d0   Section        0  stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init)
    i.HAL_GPIO_ReadPin                       0x080004c8   Section        0  stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin)
    i.HAL_GPIO_WritePin                      0x080004d2   Section        0  stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin)
    i.HAL_GetTick                            0x080004dc   Section        0  stm32f1xx_hal.o(i.HAL_GetTick)
    i.HAL_IncTick                            0x080004e8   Section        0  stm32f1xx_hal.o(i.HAL_IncTick)
    i.HAL_Init                               0x080004f8   Section        0  stm32f1xx_hal.o(i.HAL_Init)
    i.HAL_InitTick                           0x0800051c   Section        0  stm32f1xx_hal.o(i.HAL_InitTick)
    i.HAL_MspInit                            0x0800055c   Section        0  stm32f1xx_hal_msp.o(i.HAL_MspInit)
    i.HAL_NVIC_DisableIRQ                    0x08000598   Section        0  stm32f1xx_hal_cortex.o(i.HAL_NVIC_DisableIRQ)
    i.HAL_NVIC_EnableIRQ                     0x080005ba   Section        0  stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ)
    i.HAL_NVIC_SetPriority                   0x080005d4   Section        0  stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority)
    i.HAL_NVIC_SetPriorityGrouping           0x08000614   Section        0  stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping)
    i.HAL_RCC_ClockConfig                    0x08000638   Section        0  stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig)
    i.HAL_RCC_GetPCLK1Freq                   0x08000764   Section        0  stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq)
    i.HAL_RCC_GetPCLK2Freq                   0x08000784   Section        0  stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq)
    i.HAL_RCC_GetSysClockFreq                0x080007a4   Section        0  stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq)
    i.HAL_RCC_OscConfig                      0x08000810   Section        0  stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig)
    i.HAL_SPI_Init                           0x08000b30   Section        0  stm32f1xx_hal_spi.o(i.HAL_SPI_Init)
    i.HAL_SPI_MspInit                        0x08000be4   Section        0  stm32f1xx_hal_msp.o(i.HAL_SPI_MspInit)
    i.HAL_SPI_Transmit                       0x08000c54   Section        0  stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit)
    i.HAL_SPI_TransmitReceive                0x08000dba   Section        0  stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive)
    i.HAL_SYSTICK_Config                     0x08000f9c   Section        0  stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config)
    i.HAL_UART_Init                          0x08000fc4   Section        0  stm32f1xx_hal_uart.o(i.HAL_UART_Init)
    i.HAL_UART_MspInit                       0x08001028   Section        0  stm32f1xx_hal_msp.o(i.HAL_UART_MspInit)
    i.HAL_UART_Transmit                      0x08001098   Section        0  stm32f1xx_hal_uart.o(i.HAL_UART_Transmit)
    i.HardFault_Handler                      0x0800114a   Section        0  stm32f1xx_it.o(i.HardFault_Handler)
    i.LoRa_Init                              0x0800114c   Section        0  test.o(i.LoRa_Init)
    i.LoRa_Test_Handle                       0x080012b8   Section        0  test.o(i.LoRa_Test_Handle)
    i.LoRa_Test_Main                         0x080013ec   Section        0  test.o(i.LoRa_Test_Main)
    i.MX_GPIO_Init                           0x0800141c   Section        0  main.o(i.MX_GPIO_Init)
    MX_GPIO_Init                             0x0800141d   Thumb Code   196  main.o(i.MX_GPIO_Init)
    i.MX_SPI1_Init                           0x080014f0   Section        0  main.o(i.MX_SPI1_Init)
    MX_SPI1_Init                             0x080014f1   Thumb Code    58  main.o(i.MX_SPI1_Init)
    i.MemManage_Handler                      0x08001534   Section        0  stm32f1xx_it.o(i.MemManage_Handler)
    i.NMI_Handler                            0x08001536   Section        0  stm32f1xx_it.o(i.NMI_Handler)
    i.OnRxDone                               0x08001538   Section        0  test.o(i.OnRxDone)
    i.OnRxError                              0x080015b8   Section        0  test.o(i.OnRxError)
    i.OnRxTimeout                            0x080015dc   Section        0  test.o(i.OnRxTimeout)
    i.OnTxDone                               0x08001600   Section        0  test.o(i.OnTxDone)
    i.OnTxTimeout                            0x08001624   Section        0  test.o(i.OnTxTimeout)
    i.PendSV_Handler                         0x08001648   Section        0  stm32f1xx_it.o(i.PendSV_Handler)
    i.RadioAddRegisterToRetentionList        0x0800164c   Section        0  radio.o(i.RadioAddRegisterToRetentionList)
    i.RadioCheckRfFrequency                  0x080016a8   Section        0  radio.o(i.RadioCheckRfFrequency)
    i.RadioGetFskBandwidthRegValue           0x080016ac   Section        0  radio.o(i.RadioGetFskBandwidthRegValue)
    RadioGetFskBandwidthRegValue             0x080016ad   Thumb Code    48  radio.o(i.RadioGetFskBandwidthRegValue)
    i.RadioGetLoRaTimeOnAirNumerator         0x080016e0   Section        0  radio.o(i.RadioGetLoRaTimeOnAirNumerator)
    RadioGetLoRaTimeOnAirNumerator           0x080016e1   Thumb Code   122  radio.o(i.RadioGetLoRaTimeOnAirNumerator)
    i.RadioGetStatus                         0x0800175a   Section        0  radio.o(i.RadioGetStatus)
    i.RadioGetWakeupTime                     0x0800177c   Section        0  radio.o(i.RadioGetWakeupTime)
    i.RadioInit                              0x08001788   Section        0  radio.o(i.RadioInit)
    i.RadioIrqProcess                        0x080017fc   Section        0  radio.o(i.RadioIrqProcess)
    i.RadioIsChannelFree                     0x0800194c   Section        0  radio.o(i.RadioIsChannelFree)
    i.RadioOnDioIrq                          0x080019c8   Section        0  radio.o(i.RadioOnDioIrq)
    i.RadioOnRxTimeoutIrq                    0x080019d4   Section        0  radio.o(i.RadioOnRxTimeoutIrq)
    i.RadioOnTxTimeoutIrq                    0x080019ec   Section        0  radio.o(i.RadioOnTxTimeoutIrq)
    i.RadioRandom                            0x08001a04   Section        0  radio.o(i.RadioRandom)
    i.RadioRead                              0x08001a20   Section        0  radio.o(i.RadioRead)
    i.RadioReadBuffer                        0x08001a26   Section        0  radio.o(i.RadioReadBuffer)
    i.RadioRssi                              0x08001a2c   Section        0  radio.o(i.RadioRssi)
    i.RadioRx                                0x08001a30   Section        0  radio.o(i.RadioRx)
    i.RadioRxBoosted                         0x08001a74   Section        0  radio.o(i.RadioRxBoosted)
    i.RadioSend                              0x08001ab8   Section        0  radio.o(i.RadioSend)
    i.RadioSetChannel                        0x08001b10   Section        0  radio.o(i.RadioSetChannel)
    i.RadioSetMaxPayloadLength               0x08001b14   Section        0  radio.o(i.RadioSetMaxPayloadLength)
    i.RadioSetModem                          0x08001b3c   Section        0  radio.o(i.RadioSetModem)
    i.RadioSetPublicNetwork                  0x08001b6c   Section        0  radio.o(i.RadioSetPublicNetwork)
    i.RadioSetRxConfig                       0x08001ba4   Section        0  radio.o(i.RadioSetRxConfig)
    i.RadioSetRxDutyCycle                    0x08001d58   Section        0  radio.o(i.RadioSetRxDutyCycle)
    i.RadioSetTxConfig                       0x08001d5c   Section        0  radio.o(i.RadioSetTxConfig)
    i.RadioSetTxContinuousWave               0x08001ecc   Section        0  radio.o(i.RadioSetTxContinuousWave)
    i.RadioSleep                             0x08001efc   Section        0  radio.o(i.RadioSleep)
    i.RadioStandby                           0x08001f0e   Section        0  radio.o(i.RadioStandby)
    i.RadioStartCad                          0x08001f14   Section        0  radio.o(i.RadioStartCad)
    i.RadioTimeOnAir                         0x08001f2c   Section        0  radio.o(i.RadioTimeOnAir)
    i.RadioWrite                             0x08001ff8   Section        0  radio.o(i.RadioWrite)
    i.RadioWriteBuffer                       0x08001ffe   Section        0  radio.o(i.RadioWriteBuffer)
    i.SPI_EndRxTxTransaction                 0x08002004   Section        0  stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction)
    SPI_EndRxTxTransaction                   0x08002005   Thumb Code    32  stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction)
    i.SPI_WaitFlagStateUntilTimeout          0x08002024   Section        0  stm32f1xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout)
    SPI_WaitFlagStateUntilTimeout            0x08002025   Thumb Code   180  stm32f1xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout)
    i.SVC_Handler                            0x080020dc   Section        0  stm32f1xx_it.o(i.SVC_Handler)
    i.SX126xAntSwOff                         0x080020de   Section        0  sx126x-board.o(i.SX126xAntSwOff)
    i.SX126xAntSwOn                          0x080020e0   Section        0  sx126x-board.o(i.SX126xAntSwOn)
    i.SX126xCalibrateImage                   0x080020e4   Section        0  sx126x.o(i.SX126xCalibrateImage)
    i.SX126xCheckDeviceReady                 0x08002158   Section        0  sx126x.o(i.SX126xCheckDeviceReady)
    i.SX126xClearIrqStatus                   0x08002178   Section        0  sx126x.o(i.SX126xClearIrqStatus)
    i.SX126xConvertFreqInHzToPllStep         0x08002190   Section        0  sx126x.o(i.SX126xConvertFreqInHzToPllStep)
    SX126xConvertFreqInHzToPllStep           0x08002191   Thumb Code    30  sx126x.o(i.SX126xConvertFreqInHzToPllStep)
    i.SX126xDbgPinRxWrite                    0x080021b0   Section        0  sx126x-board.o(i.SX126xDbgPinRxWrite)
    SX126xDbgPinRxWrite                      0x080021b1   Thumb Code    18  sx126x-board.o(i.SX126xDbgPinRxWrite)
    i.SX126xDbgPinTxWrite                    0x080021c8   Section        0  sx126x-board.o(i.SX126xDbgPinTxWrite)
    SX126xDbgPinTxWrite                      0x080021c9   Thumb Code    18  sx126x-board.o(i.SX126xDbgPinTxWrite)
    i.SX126xGetBoardTcxoWakeupTime           0x080021e0   Section        0  sx126x-board.o(i.SX126xGetBoardTcxoWakeupTime)
    i.SX126xGetDeviceId                      0x080021e4   Section        0  sx126x-board.o(i.SX126xGetDeviceId)
    i.SX126xGetDio1PinState                  0x080021e8   Section        0  sx126x-board.o(i.SX126xGetDio1PinState)
    i.SX126xGetIrqStatus                     0x08002200   Section        0  sx126x.o(i.SX126xGetIrqStatus)
    i.SX126xGetOperatingMode                 0x08002214   Section        0  sx126x-board.o(i.SX126xGetOperatingMode)
    i.SX126xGetPacketStatus                  0x08002220   Section        0  sx126x.o(i.SX126xGetPacketStatus)
    i.SX126xGetPacketType                    0x08002290   Section        0  sx126x.o(i.SX126xGetPacketType)
    i.SX126xGetPayload                       0x0800229c   Section        0  sx126x.o(i.SX126xGetPayload)
    i.SX126xGetRandom                        0x080022ca   Section        0  sx126x.o(i.SX126xGetRandom)
    i.SX126xGetRssiInst                      0x08002328   Section        0  sx126x.o(i.SX126xGetRssiInst)
    i.SX126xGetRxBufferStatus                0x08002340   Section        0  sx126x.o(i.SX126xGetRxBufferStatus)
    i.SX126xInit                             0x0800237c   Section        0  sx126x.o(i.SX126xInit)
    i.SX126xIoInit                           0x080023b4   Section        0  sx126x-board.o(i.SX126xIoInit)
    i.SX126xIoIrqInit                        0x08002460   Section        0  sx126x-board.o(i.SX126xIoIrqInit)
    i.SX126xIoRfSwitchInit                   0x0800248c   Section        0  sx126x-board.o(i.SX126xIoRfSwitchInit)
    i.SX126xIoTcxoInit                       0x08002492   Section        0  sx126x-board.o(i.SX126xIoTcxoInit)
    i.SX126xReadBuffer                       0x08002494   Section        0  sx126x-board.o(i.SX126xReadBuffer)
    i.SX126xReadCommand                      0x08002500   Section        0  sx126x-board.o(i.SX126xReadCommand)
    i.SX126xReadRegister                     0x08002568   Section        0  sx126x-board.o(i.SX126xReadRegister)
    i.SX126xReadRegisters                    0x08002578   Section        0  sx126x-board.o(i.SX126xReadRegisters)
    i.SX126xReset                            0x080025ec   Section        0  sx126x-board.o(i.SX126xReset)
    i.SX126xSendPayload                      0x08002620   Section        0  sx126x.o(i.SX126xSendPayload)
    i.SX126xSetBufferBaseAddress             0x08002632   Section        0  sx126x.o(i.SX126xSetBufferBaseAddress)
    i.SX126xSetCad                           0x08002648   Section        0  sx126x.o(i.SX126xSetCad)
    i.SX126xSetCrcPolynomial                 0x08002660   Section        0  sx126x.o(i.SX126xSetCrcPolynomial)
    i.SX126xSetCrcSeed                       0x08002688   Section        0  sx126x.o(i.SX126xSetCrcSeed)
    i.SX126xSetDio2AsRfSwitchCtrl            0x080026b0   Section        0  sx126x.o(i.SX126xSetDio2AsRfSwitchCtrl)
    i.SX126xSetDioIrqParams                  0x080026be   Section        0  sx126x.o(i.SX126xSetDioIrqParams)
    i.SX126xSetLoRaSymbNumTimeout            0x080026f4   Section        0  sx126x.o(i.SX126xSetLoRaSymbNumTimeout)
    i.SX126xSetModulationParams              0x08002748   Section        0  sx126x.o(i.SX126xSetModulationParams)
    i.SX126xSetOperatingMode                 0x080027d4   Section        0  sx126x-board.o(i.SX126xSetOperatingMode)
    i.SX126xSetPaConfig                      0x0800280c   Section        0  sx126x.o(i.SX126xSetPaConfig)
    i.SX126xSetPacketParams                  0x0800282c   Section        0  sx126x.o(i.SX126xSetPacketParams)
    i.SX126xSetPacketType                    0x080028f0   Section        0  sx126x.o(i.SX126xSetPacketType)
    i.SX126xSetPayload                       0x0800290c   Section        0  sx126x.o(i.SX126xSetPayload)
    i.SX126xSetRegulatorMode                 0x08002916   Section        0  sx126x.o(i.SX126xSetRegulatorMode)
    i.SX126xSetRfFrequency                   0x08002924   Section        0  sx126x.o(i.SX126xSetRfFrequency)
    i.SX126xSetRfTxPower                     0x08002964   Section        0  sx126x-board.o(i.SX126xSetRfTxPower)
    i.SX126xSetRx                            0x0800296a   Section        0  sx126x.o(i.SX126xSetRx)
    i.SX126xSetRxBoosted                     0x0800299a   Section        0  sx126x.o(i.SX126xSetRxBoosted)
    i.SX126xSetRxDutyCycle                   0x080029ca   Section        0  sx126x.o(i.SX126xSetRxDutyCycle)
    i.SX126xSetSleep                         0x08002a00   Section        0  sx126x.o(i.SX126xSetSleep)
    i.SX126xSetStandby                       0x08002a40   Section        0  sx126x.o(i.SX126xSetStandby)
    i.SX126xSetStopRxTimerOnPreambleDetect   0x08002a5e   Section        0  sx126x.o(i.SX126xSetStopRxTimerOnPreambleDetect)
    i.SX126xSetSyncWord                      0x08002a6c   Section        0  sx126x.o(i.SX126xSetSyncWord)
    i.SX126xSetTx                            0x08002a7e   Section        0  sx126x.o(i.SX126xSetTx)
    i.SX126xSetTxContinuousWave              0x08002aa4   Section        0  sx126x.o(i.SX126xSetTxContinuousWave)
    i.SX126xSetTxParams                      0x08002aba   Section        0  sx126x.o(i.SX126xSetTxParams)
    i.SX126xSetWhiteningSeed                 0x08002b38   Section        0  sx126x.o(i.SX126xSetWhiteningSeed)
    i.SX126xWaitOnBusy                       0x08002b70   Section        0  sx126x-board.o(i.SX126xWaitOnBusy)
    i.SX126xWakeup                           0x08002b88   Section        0  sx126x-board.o(i.SX126xWakeup)
    i.SX126xWriteBuffer                      0x08002bd4   Section        0  sx126x-board.o(i.SX126xWriteBuffer)
    i.SX126xWriteCommand                     0x08002c2c   Section        0  sx126x-board.o(i.SX126xWriteCommand)
    i.SX126xWriteRegister                    0x08002c88   Section        0  sx126x-board.o(i.SX126xWriteRegister)
    i.SX126xWriteRegisters                   0x08002c94   Section        0  sx126x-board.o(i.SX126xWriteRegisters)
    i.SysTick_Handler                        0x08002cf4   Section        0  stm32f1xx_it.o(i.SysTick_Handler)
    i.SystemClock_Config                     0x08002cf8   Section        0  main.o(i.SystemClock_Config)
    i.SystemInit                             0x08002d54   Section        0  system_stm32f1xx.o(i.SystemInit)
    i.TimerGetCurrentTime                    0x08002d56   Section        0  timer.o(i.TimerGetCurrentTime)
    i.TimerGetElapsedTime                    0x08002d5a   Section        0  timer.o(i.TimerGetElapsedTime)
    i.TimerInit                              0x08002d68   Section        0  timer.o(i.TimerInit)
    i.TimerService                           0x08002d94   Section        0  timer.o(i.TimerService)
    i.TimerSetValue                          0x08002de4   Section        0  timer.o(i.TimerSetValue)
    i.TimerStart                             0x08002df0   Section        0  timer.o(i.TimerStart)
    i.TimerStop                              0x08002e08   Section        0  timer.o(i.TimerStop)
    i.UART_SetConfig                         0x08002e14   Section        0  stm32f1xx_hal_uart.o(i.UART_SetConfig)
    UART_SetConfig                           0x08002e15   Thumb Code   178  stm32f1xx_hal_uart.o(i.UART_SetConfig)
    i.UART_WaitOnFlagUntilTimeout            0x08002ecc   Section        0  stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout)
    UART_WaitOnFlagUntilTimeout              0x08002ecd   Thumb Code   100  stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout)
    i.UsageFault_Handler                     0x08002f30   Section        0  stm32f1xx_it.o(i.UsageFault_Handler)
    i.__0printf$8                            0x08002f34   Section        0  printf8.o(i.__0printf$8)
    i.__NVIC_SetPriority                     0x08002f54   Section        0  stm32f1xx_hal_cortex.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x08002f55   Thumb Code    32  stm32f1xx_hal_cortex.o(i.__NVIC_SetPriority)
    i.__scatterload_copy                     0x08002f74   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x08002f82   Section        2  handlers.o(i.__scatterload_null)
    i.__scatterload_zeroinit                 0x08002f84   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._printf_core                           0x08002f94   Section        0  printf8.o(i._printf_core)
    _printf_core                             0x08002f95   Thumb Code   996  printf8.o(i._printf_core)
    i._printf_post_padding                   0x080033a4   Section        0  printf8.o(i._printf_post_padding)
    _printf_post_padding                     0x080033a5   Thumb Code    36  printf8.o(i._printf_post_padding)
    i._printf_pre_padding                    0x080033c8   Section        0  printf8.o(i._printf_pre_padding)
    _printf_pre_padding                      0x080033c9   Thumb Code    46  printf8.o(i._printf_pre_padding)
    i.fputc                                  0x080033f8   Section        0  main.o(i.fputc)
    i.main                                   0x08003414   Section        0  main.o(i.main)
    .constdata                               0x08003474   Section       16  system_stm32f1xx.o(.constdata)
    .constdata                               0x08003484   Section        8  system_stm32f1xx.o(.constdata)
    .constdata                               0x0800348c   Section      108  radio.o(.constdata)
    .constdata                               0x080034f8   Section      180  radio.o(.constdata)
    .data                                    0x20000000   Section       12  stm32f1xx_hal.o(.data)
    .data                                    0x2000000c   Section        4  system_stm32f1xx.o(.data)
    .data                                    0x20000010   Section        8  sx126x-board.o(.data)
    LoRaIOInitFlag                           0x20000010   Data           1  sx126x-board.o(.data)
    OperatingMode                            0x20000011   Data           1  sx126x-board.o(.data)
    .data                                    0x20000018   Section        4  timer.o(.data)
    systick_local                            0x20000018   Data           4  timer.o(.data)
    .data                                    0x2000001c   Section       20  radio.o(.data)
    RadioPublicNetwork                       0x2000001f   Data           2  radio.o(.data)
    RadioEvents                              0x2000002c   Data           4  radio.o(.data)
    .data                                    0x20000030   Section        8  sx126x.o(.data)
    ImageCalibrated                          0x20000030   Data           1  sx126x.o(.data)
    PacketType                               0x20000031   Data           1  sx126x.o(.data)
    LoRaHeaderType                           0x20000032   Data           1  sx126x.o(.data)
    .data                                    0x20000038   Section        1  test.o(.data)
    test_cnt                                 0x20000038   Data           1  test.o(.data)
    .data                                    0x2000003c   Section        4  stdout.o(.data)
    .bss                                     0x20000040   Section      156  main.o(.bss)
    .bss                                     0x200000dc   Section      520  sx126x-board.o(.bss)
    .bss                                     0x200002e4   Section       24  timer.o(.bss)
    timer_head_ptr                           0x200002e4   Data          24  timer.o(.bss)
    .bss                                     0x200002fc   Section      384  radio.o(.bss)
    .bss                                     0x2000047c   Section      572  test.o(.bss)
    RadioEvents                              0x2000047c   Data          36  test.o(.bss)
    STACK                                    0x200006b8   Section     1024  startup_stm32f103xe.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv4$P$D$K$B$S$PE$A:L22UL41UL21$X:L11$S22US41US21$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OSPACE$ROPI$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    __decompress                              - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x00000130   Number         0  startup_stm32f103xe.o ABSOLUTE
    __Vectors                                0x08000000   Data           4  startup_stm32f103xe.o(RESET)
    __Vectors_End                            0x08000130   Data           0  startup_stm32f103xe.o(RESET)
    __main                                   0x08000131   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x08000131   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x08000135   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x08000139   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x08000139   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x08000139   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x08000139   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x08000141   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x08000141   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x08000145   Thumb Code     8  startup_stm32f103xe.o(.text)
    ADC1_2_IRQHandler                        0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    ADC3_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    CAN1_RX1_IRQHandler                      0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    CAN1_SCE_IRQHandler                      0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA1_Channel1_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA1_Channel2_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA1_Channel3_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA1_Channel4_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA1_Channel5_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA1_Channel6_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA1_Channel7_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA2_Channel1_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA2_Channel2_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA2_Channel3_IRQHandler                 0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    DMA2_Channel4_5_IRQHandler               0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    EXTI15_10_IRQHandler                     0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    EXTI1_IRQHandler                         0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    EXTI2_IRQHandler                         0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    EXTI3_IRQHandler                         0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    EXTI4_IRQHandler                         0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    EXTI9_5_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    FLASH_IRQHandler                         0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    FSMC_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    I2C1_ER_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    I2C1_EV_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    I2C2_ER_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    I2C2_EV_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    PVD_IRQHandler                           0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    RCC_IRQHandler                           0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    RTC_Alarm_IRQHandler                     0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    RTC_IRQHandler                           0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    SDIO_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    SPI1_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    SPI2_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    SPI3_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TAMPER_IRQHandler                        0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM1_BRK_IRQHandler                      0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM1_CC_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM1_TRG_COM_IRQHandler                  0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM1_UP_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM2_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM3_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM4_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM5_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM6_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM7_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM8_BRK_IRQHandler                      0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM8_CC_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM8_TRG_COM_IRQHandler                  0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    TIM8_UP_IRQHandler                       0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    UART4_IRQHandler                         0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    UART5_IRQHandler                         0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    USART1_IRQHandler                        0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    USART2_IRQHandler                        0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    USART3_IRQHandler                        0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    USBWakeUp_IRQHandler                     0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    USB_HP_CAN1_TX_IRQHandler                0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    USB_LP_CAN1_RX0_IRQHandler               0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    WWDG_IRQHandler                          0x0800015f   Thumb Code     0  startup_stm32f103xe.o(.text)
    __aeabi_llsr                             0x08000169   Thumb Code    32  llushr.o(.text)
    _ll_ushift_r                             0x08000169   Thumb Code     0  llushr.o(.text)
    __aeabi_memcpy                           0x08000189   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x08000189   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x08000189   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x080001ad   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x080001ad   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x080001ad   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x080001bb   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x080001bb   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x080001bb   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x080001bf   Thumb Code    18  memseta.o(.text)
    __aeabi_uldivmod                         0x080001d1   Thumb Code    98  uldiv.o(.text)
    __scatterload                            0x08000235   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x08000235   Thumb Code     0  init.o(.text)
    __aeabi_llsl                             0x08000259   Thumb Code    30  llshl.o(.text)
    _ll_shift_l                              0x08000259   Thumb Code     0  llshl.o(.text)
    BusFault_Handler                         0x08000277   Thumb Code     2  stm32f1xx_it.o(i.BusFault_Handler)
    DebugMon_Handler                         0x08000279   Thumb Code     2  stm32f1xx_it.o(i.DebugMon_Handler)
    DelayMs                                  0x0800027d   Thumb Code    24  timer.o(i.DelayMs)
    EXTI0_IRQHandler                         0x08000295   Thumb Code     6  stm32f1xx_it.o(i.EXTI0_IRQHandler)
    HAL_GPIO_EXTI_Callback                   0x0800029d   Thumb Code    24  sx126x-board.o(i.HAL_GPIO_EXTI_Callback)
    HAL_GPIO_EXTI_IRQHandler                 0x080002b9   Thumb Code    18  stm32f1xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler)
    HAL_GPIO_Init                            0x080002d1   Thumb Code   462  stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init)
    HAL_GPIO_ReadPin                         0x080004c9   Thumb Code    10  stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin)
    HAL_GPIO_WritePin                        0x080004d3   Thumb Code    10  stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin)
    HAL_GetTick                              0x080004dd   Thumb Code     6  stm32f1xx_hal.o(i.HAL_GetTick)
    HAL_IncTick                              0x080004e9   Thumb Code    12  stm32f1xx_hal.o(i.HAL_IncTick)
    HAL_Init                                 0x080004f9   Thumb Code    32  stm32f1xx_hal.o(i.HAL_Init)
    HAL_InitTick                             0x0800051d   Thumb Code    54  stm32f1xx_hal.o(i.HAL_InitTick)
    HAL_MspInit                              0x0800055d   Thumb Code    52  stm32f1xx_hal_msp.o(i.HAL_MspInit)
    HAL_NVIC_DisableIRQ                      0x08000599   Thumb Code    34  stm32f1xx_hal_cortex.o(i.HAL_NVIC_DisableIRQ)
    HAL_NVIC_EnableIRQ                       0x080005bb   Thumb Code    26  stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ)
    HAL_NVIC_SetPriority                     0x080005d5   Thumb Code    60  stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority)
    HAL_NVIC_SetPriorityGrouping             0x08000615   Thumb Code    26  stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping)
    HAL_RCC_ClockConfig                      0x08000639   Thumb Code   280  stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig)
    HAL_RCC_GetPCLK1Freq                     0x08000765   Thumb Code    20  stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq)
    HAL_RCC_GetPCLK2Freq                     0x08000785   Thumb Code    20  stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq)
    HAL_RCC_GetSysClockFreq                  0x080007a5   Thumb Code    74  stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq)
    HAL_RCC_OscConfig                        0x08000811   Thumb Code   778  stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig)
    HAL_SPI_Init                             0x08000b31   Thumb Code   178  stm32f1xx_hal_spi.o(i.HAL_SPI_Init)
    HAL_SPI_MspInit                          0x08000be5   Thumb Code    98  stm32f1xx_hal_msp.o(i.HAL_SPI_MspInit)
    HAL_SPI_Transmit                         0x08000c55   Thumb Code   358  stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit)
    HAL_SPI_TransmitReceive                  0x08000dbb   Thumb Code   482  stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive)
    HAL_SYSTICK_Config                       0x08000f9d   Thumb Code    40  stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config)
    HAL_UART_Init                            0x08000fc5   Thumb Code    98  stm32f1xx_hal_uart.o(i.HAL_UART_Init)
    HAL_UART_MspInit                         0x08001029   Thumb Code   100  stm32f1xx_hal_msp.o(i.HAL_UART_MspInit)
    HAL_UART_Transmit                        0x08001099   Thumb Code   178  stm32f1xx_hal_uart.o(i.HAL_UART_Transmit)
    HardFault_Handler                        0x0800114b   Thumb Code     2  stm32f1xx_it.o(i.HardFault_Handler)
    LoRa_Init                                0x0800114d   Thumb Code   202  test.o(i.LoRa_Init)
    LoRa_Test_Handle                         0x080012b9   Thumb Code   144  test.o(i.LoRa_Test_Handle)
    LoRa_Test_Main                           0x080013ed   Thumb Code    36  test.o(i.LoRa_Test_Main)
    MemManage_Handler                        0x08001535   Thumb Code     2  stm32f1xx_it.o(i.MemManage_Handler)
    NMI_Handler                              0x08001537   Thumb Code     2  stm32f1xx_it.o(i.NMI_Handler)
    OnRxDone                                 0x08001539   Thumb Code    72  test.o(i.OnRxDone)
    OnRxError                                0x080015b9   Thumb Code    20  test.o(i.OnRxError)
    OnRxTimeout                              0x080015dd   Thumb Code    20  test.o(i.OnRxTimeout)
    OnTxDone                                 0x08001601   Thumb Code    20  test.o(i.OnTxDone)
    OnTxTimeout                              0x08001625   Thumb Code    20  test.o(i.OnTxTimeout)
    PendSV_Handler                           0x08001649   Thumb Code     2  stm32f1xx_it.o(i.PendSV_Handler)
    RadioAddRegisterToRetentionList          0x0800164d   Thumb Code    92  radio.o(i.RadioAddRegisterToRetentionList)
    RadioCheckRfFrequency                    0x080016a9   Thumb Code     4  radio.o(i.RadioCheckRfFrequency)
    RadioGetStatus                           0x0800175b   Thumb Code    34  radio.o(i.RadioGetStatus)
    RadioGetWakeupTime                       0x0800177d   Thumb Code    10  radio.o(i.RadioGetWakeupTime)
    RadioInit                                0x08001789   Thumb Code    94  radio.o(i.RadioInit)
    RadioIrqProcess                          0x080017fd   Thumb Code   322  radio.o(i.RadioIrqProcess)
    RadioIsChannelFree                       0x0800194d   Thumb Code   122  radio.o(i.RadioIsChannelFree)
    RadioOnDioIrq                            0x080019c9   Thumb Code     8  radio.o(i.RadioOnDioIrq)
    RadioOnRxTimeoutIrq                      0x080019d5   Thumb Code    18  radio.o(i.RadioOnRxTimeoutIrq)
    RadioOnTxTimeoutIrq                      0x080019ed   Thumb Code    18  radio.o(i.RadioOnTxTimeoutIrq)
    RadioRandom                              0x08001a05   Thumb Code    28  radio.o(i.RadioRandom)
    RadioRead                                0x08001a21   Thumb Code     6  radio.o(i.RadioRead)
    RadioReadBuffer                          0x08001a27   Thumb Code     6  radio.o(i.RadioReadBuffer)
    RadioRssi                                0x08001a2d   Thumb Code     4  radio.o(i.RadioRssi)
    RadioRx                                  0x08001a31   Thumb Code    58  radio.o(i.RadioRx)
    RadioRxBoosted                           0x08001a75   Thumb Code    58  radio.o(i.RadioRxBoosted)
    RadioSend                                0x08001ab9   Thumb Code    78  radio.o(i.RadioSend)
    RadioSetChannel                          0x08001b11   Thumb Code     4  radio.o(i.RadioSetChannel)
    RadioSetMaxPayloadLength                 0x08001b15   Thumb Code    32  radio.o(i.RadioSetMaxPayloadLength)
    RadioSetModem                            0x08001b3d   Thumb Code    44  radio.o(i.RadioSetModem)
    RadioSetPublicNetwork                    0x08001b6d   Thumb Code    52  radio.o(i.RadioSetPublicNetwork)
    RadioSetRxConfig                         0x08001ba5   Thumb Code   416  radio.o(i.RadioSetRxConfig)
    RadioSetRxDutyCycle                      0x08001d59   Thumb Code     4  radio.o(i.RadioSetRxDutyCycle)
    RadioSetTxConfig                         0x08001d5d   Thumb Code   348  radio.o(i.RadioSetTxConfig)
    RadioSetTxContinuousWave                 0x08001ecd   Thumb Code    44  radio.o(i.RadioSetTxContinuousWave)
    RadioSleep                               0x08001efd   Thumb Code    18  radio.o(i.RadioSleep)
    RadioStandby                             0x08001f0f   Thumb Code     6  radio.o(i.RadioStandby)
    RadioStartCad                            0x08001f15   Thumb Code    24  radio.o(i.RadioStartCad)
    RadioTimeOnAir                           0x08001f2d   Thumb Code   186  radio.o(i.RadioTimeOnAir)
    RadioWrite                               0x08001ff9   Thumb Code     6  radio.o(i.RadioWrite)
    RadioWriteBuffer                         0x08001fff   Thumb Code     6  radio.o(i.RadioWriteBuffer)
    SVC_Handler                              0x080020dd   Thumb Code     2  stm32f1xx_it.o(i.SVC_Handler)
    SX126xAntSwOff                           0x080020df   Thumb Code     2  sx126x-board.o(i.SX126xAntSwOff)
    SX126xAntSwOn                            0x080020e1   Thumb Code     2  sx126x-board.o(i.SX126xAntSwOn)
    SX126xCalibrateImage                     0x080020e5   Thumb Code    96  sx126x.o(i.SX126xCalibrateImage)
    SX126xCheckDeviceReady                   0x08002159   Thumb Code    32  sx126x.o(i.SX126xCheckDeviceReady)
    SX126xClearIrqStatus                     0x08002179   Thumb Code    24  sx126x.o(i.SX126xClearIrqStatus)
    SX126xGetBoardTcxoWakeupTime             0x080021e1   Thumb Code     4  sx126x-board.o(i.SX126xGetBoardTcxoWakeupTime)
    SX126xGetDeviceId                        0x080021e5   Thumb Code     4  sx126x-board.o(i.SX126xGetDeviceId)
    SX126xGetDio1PinState                    0x080021e9   Thumb Code    18  sx126x-board.o(i.SX126xGetDio1PinState)
    SX126xGetIrqStatus                       0x08002201   Thumb Code    20  sx126x.o(i.SX126xGetIrqStatus)
    SX126xGetOperatingMode                   0x08002215   Thumb Code     6  sx126x-board.o(i.SX126xGetOperatingMode)
    SX126xGetPacketStatus                    0x08002221   Thumb Code   108  sx126x.o(i.SX126xGetPacketStatus)
    SX126xGetPacketType                      0x08002291   Thumb Code     6  sx126x.o(i.SX126xGetPacketType)
    SX126xGetPayload                         0x0800229d   Thumb Code    46  sx126x.o(i.SX126xGetPayload)
    SX126xGetRandom                          0x080022cb   Thumb Code    94  sx126x.o(i.SX126xGetRandom)
    SX126xGetRssiInst                        0x08002329   Thumb Code    24  sx126x.o(i.SX126xGetRssiInst)
    SX126xGetRxBufferStatus                  0x08002341   Thumb Code    54  sx126x.o(i.SX126xGetRxBufferStatus)
    SX126xInit                               0x0800237d   Thumb Code    52  sx126x.o(i.SX126xInit)
    SX126xIoInit                             0x080023b5   Thumb Code   154  sx126x-board.o(i.SX126xIoInit)
    SX126xIoIrqInit                          0x08002461   Thumb Code    38  sx126x-board.o(i.SX126xIoIrqInit)
    SX126xIoRfSwitchInit                     0x0800248d   Thumb Code     6  sx126x-board.o(i.SX126xIoRfSwitchInit)
    SX126xIoTcxoInit                         0x08002493   Thumb Code     2  sx126x-board.o(i.SX126xIoTcxoInit)
    SX126xReadBuffer                         0x08002495   Thumb Code    90  sx126x-board.o(i.SX126xReadBuffer)
    SX126xReadCommand                        0x08002501   Thumb Code    88  sx126x-board.o(i.SX126xReadCommand)
    SX126xReadRegister                       0x08002569   Thumb Code    16  sx126x-board.o(i.SX126xReadRegister)
    SX126xReadRegisters                      0x08002579   Thumb Code    98  sx126x-board.o(i.SX126xReadRegisters)
    SX126xReset                              0x080025ed   Thumb Code    46  sx126x-board.o(i.SX126xReset)
    SX126xSendPayload                        0x08002621   Thumb Code    18  sx126x.o(i.SX126xSendPayload)
    SX126xSetBufferBaseAddress               0x08002633   Thumb Code    22  sx126x.o(i.SX126xSetBufferBaseAddress)
    SX126xSetCad                             0x08002649   Thumb Code    22  sx126x.o(i.SX126xSetCad)
    SX126xSetCrcPolynomial                   0x08002661   Thumb Code    34  sx126x.o(i.SX126xSetCrcPolynomial)
    SX126xSetCrcSeed                         0x08002689   Thumb Code    34  sx126x.o(i.SX126xSetCrcSeed)
    SX126xSetDio2AsRfSwitchCtrl              0x080026b1   Thumb Code    14  sx126x.o(i.SX126xSetDio2AsRfSwitchCtrl)
    SX126xSetDioIrqParams                    0x080026bf   Thumb Code    54  sx126x.o(i.SX126xSetDioIrqParams)
    SX126xSetLoRaSymbNumTimeout              0x080026f5   Thumb Code    82  sx126x.o(i.SX126xSetLoRaSymbNumTimeout)
    SX126xSetModulationParams                0x08002749   Thumb Code   132  sx126x.o(i.SX126xSetModulationParams)
    SX126xSetOperatingMode                   0x080027d5   Thumb Code    52  sx126x-board.o(i.SX126xSetOperatingMode)
    SX126xSetPaConfig                        0x0800280d   Thumb Code    30  sx126x.o(i.SX126xSetPaConfig)
    SX126xSetPacketParams                    0x0800282d   Thumb Code   192  sx126x.o(i.SX126xSetPacketParams)
    SX126xSetPacketType                      0x080028f1   Thumb Code    22  sx126x.o(i.SX126xSetPacketType)
    SX126xSetPayload                         0x0800290d   Thumb Code    10  sx126x.o(i.SX126xSetPayload)
    SX126xSetRegulatorMode                   0x08002917   Thumb Code    14  sx126x.o(i.SX126xSetRegulatorMode)
    SX126xSetRfFrequency                     0x08002925   Thumb Code    60  sx126x.o(i.SX126xSetRfFrequency)
    SX126xSetRfTxPower                       0x08002965   Thumb Code     6  sx126x-board.o(i.SX126xSetRfTxPower)
    SX126xSetRx                              0x0800296b   Thumb Code    48  sx126x.o(i.SX126xSetRx)
    SX126xSetRxBoosted                       0x0800299b   Thumb Code    48  sx126x.o(i.SX126xSetRxBoosted)
    SX126xSetRxDutyCycle                     0x080029cb   Thumb Code    52  sx126x.o(i.SX126xSetRxDutyCycle)
    SX126xSetSleep                           0x08002a01   Thumb Code    60  sx126x.o(i.SX126xSetSleep)
    SX126xSetStandby                         0x08002a41   Thumb Code    30  sx126x.o(i.SX126xSetStandby)
    SX126xSetStopRxTimerOnPreambleDetect     0x08002a5f   Thumb Code    14  sx126x.o(i.SX126xSetStopRxTimerOnPreambleDetect)
    SX126xSetSyncWord                        0x08002a6d   Thumb Code    18  sx126x.o(i.SX126xSetSyncWord)
    SX126xSetTx                              0x08002a7f   Thumb Code    38  sx126x.o(i.SX126xSetTx)
    SX126xSetTxContinuousWave                0x08002aa5   Thumb Code    22  sx126x.o(i.SX126xSetTxContinuousWave)
    SX126xSetTxParams                        0x08002abb   Thumb Code   126  sx126x.o(i.SX126xSetTxParams)
    SX126xSetWhiteningSeed                   0x08002b39   Thumb Code    52  sx126x.o(i.SX126xSetWhiteningSeed)
    SX126xWaitOnBusy                         0x08002b71   Thumb Code    18  sx126x-board.o(i.SX126xWaitOnBusy)
    SX126xWakeup                             0x08002b89   Thumb Code    62  sx126x-board.o(i.SX126xWakeup)
    SX126xWriteBuffer                        0x08002bd5   Thumb Code    76  sx126x-board.o(i.SX126xWriteBuffer)
    SX126xWriteCommand                       0x08002c2d   Thumb Code    78  sx126x-board.o(i.SX126xWriteCommand)
    SX126xWriteRegister                      0x08002c89   Thumb Code    12  sx126x-board.o(i.SX126xWriteRegister)
    SX126xWriteRegisters                     0x08002c95   Thumb Code    84  sx126x-board.o(i.SX126xWriteRegisters)
    SysTick_Handler                          0x08002cf5   Thumb Code     4  stm32f1xx_it.o(i.SysTick_Handler)
    SystemClock_Config                       0x08002cf9   Thumb Code    92  main.o(i.SystemClock_Config)
    SystemInit                               0x08002d55   Thumb Code     2  system_stm32f1xx.o(i.SystemInit)
    TimerGetCurrentTime                      0x08002d57   Thumb Code     4  timer.o(i.TimerGetCurrentTime)
    TimerGetElapsedTime                      0x08002d5b   Thumb Code    12  timer.o(i.TimerGetElapsedTime)
    TimerInit                                0x08002d69   Thumb Code    38  timer.o(i.TimerInit)
    TimerService                             0x08002d95   Thumb Code    70  timer.o(i.TimerService)
    TimerSetValue                            0x08002de5   Thumb Code    12  timer.o(i.TimerSetValue)
    TimerStart                               0x08002df1   Thumb Code    24  timer.o(i.TimerStart)
    TimerStop                                0x08002e09   Thumb Code    10  timer.o(i.TimerStop)
    UsageFault_Handler                       0x08002f31   Thumb Code     2  stm32f1xx_it.o(i.UsageFault_Handler)
    __0printf$8                              0x08002f35   Thumb Code    22  printf8.o(i.__0printf$8)
    __1printf$8                              0x08002f35   Thumb Code     0  printf8.o(i.__0printf$8)
    __2printf                                0x08002f35   Thumb Code     0  printf8.o(i.__0printf$8)
    __scatterload_copy                       0x08002f75   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x08002f83   Thumb Code     2  handlers.o(i.__scatterload_null)
    __scatterload_zeroinit                   0x08002f85   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    fputc                                    0x080033f9   Thumb Code    24  main.o(i.fputc)
    main                                     0x08003415   Thumb Code    70  main.o(i.main)
    AHBPrescTable                            0x08003474   Data          16  system_stm32f1xx.o(.constdata)
    APBPrescTable                            0x08003484   Data           8  system_stm32f1xx.o(.constdata)
    Radio                                    0x0800348c   Data         108  radio.o(.constdata)
    Bandwidths                               0x080034f8   Data           4  radio.o(.constdata)
    FskBandwidths                            0x080034fc   Data         176  radio.o(.constdata)
    Region$$Table$$Base                      0x080035ac   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x080035cc   Number         0  anon$$obj.o(Region$$Table)
    uwTickFreq                               0x20000000   Data           1  stm32f1xx_hal.o(.data)
    uwTickPrio                               0x20000004   Data           4  stm32f1xx_hal.o(.data)
    uwTick                                   0x20000008   Data           4  stm32f1xx_hal.o(.data)
    SystemCoreClock                          0x2000000c   Data           4  system_stm32f1xx.o(.data)
    DIOx_IRQ_Function                        0x20000014   Data           4  sx126x-board.o(.data)
    MaxPayloadLength                         0x2000001c   Data           1  radio.o(.data)
    RxContinuous                             0x2000001d   Data           1  radio.o(.data)
    IrqFired                                 0x2000001e   Data           1  radio.o(.data)
    TxTimeout                                0x20000024   Data           4  radio.o(.data)
    RxTimeout                                0x20000028   Data           4  radio.o(.data)
    FrequencyError                           0x20000034   Data           4  sx126x.o(.data)
    __stdout                                 0x2000003c   Data           4  stdout.o(.data)
    hspi1                                    0x20000040   Data          88  main.o(.bss)
    huart1                                   0x20000098   Data          68  main.o(.bss)
    SPI_WriteBuffer                          0x200000dc   Data         260  sx126x-board.o(.bss)
    SPI_ReadBuffer                           0x200001e0   Data         260  sx126x-board.o(.bss)
    RadioPktStatus                           0x200002fc   Data          20  radio.o(.bss)
    RadioRxPayload                           0x20000310   Data         255  radio.o(.bss)
    SX126x                                   0x20000410   Data          60  radio.o(.bss)
    TxTimeoutTimer                           0x2000044c   Data          24  radio.o(.bss)
    RxTimeoutTimer                           0x20000464   Data          24  radio.o(.bss)
    LoRa_TX_buffer                           0x200004a0   Data         255  test.o(.bss)
    LoRa_RX_buffer                           0x2000059f   Data         255  test.o(.bss)
    TestTimer                                0x200006a0   Data          24  test.o(.bss)
    __initial_sp                             0x20000ab8   Data           0  startup_stm32f103xe.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x08000131

  Load Region LR_IROM1 (Base: 0x08000000, Size: 0x0000360c, Max: 0x00080000, ABSOLUTE)

    Execution Region ER_IROM1 (Exec base: 0x08000000, Load base: 0x08000000, Size: 0x000035cc, Max: 0x00080000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x08000000   0x08000000   0x00000130   Data   RO            3    RESET               startup_stm32f103xe.o
    0x08000130   0x08000130   0x00000000   Code   RO         2971  * .ARM.Collect$$$$00000000  mc_w.l(entry.o)
    0x08000130   0x08000130   0x00000004   Code   RO         3243    .ARM.Collect$$$$00000001  mc_w.l(entry2.o)
    0x08000134   0x08000134   0x00000004   Code   RO         3246    .ARM.Collect$$$$00000004  mc_w.l(entry5.o)
    0x08000138   0x08000138   0x00000000   Code   RO         3248    .ARM.Collect$$$$00000008  mc_w.l(entry7b.o)
    0x08000138   0x08000138   0x00000000   Code   RO         3250    .ARM.Collect$$$$0000000A  mc_w.l(entry8b.o)
    0x08000138   0x08000138   0x00000008   Code   RO         3251    .ARM.Collect$$$$0000000B  mc_w.l(entry9a.o)
    0x08000140   0x08000140   0x00000000   Code   RO         3253    .ARM.Collect$$$$0000000D  mc_w.l(entry10a.o)
    0x08000140   0x08000140   0x00000000   Code   RO         3255    .ARM.Collect$$$$0000000F  mc_w.l(entry11a.o)
    0x08000140   0x08000140   0x00000004   Code   RO         3244    .ARM.Collect$$$$00002712  mc_w.l(entry2.o)
    0x08000144   0x08000144   0x00000024   Code   RO            4    .text               startup_stm32f103xe.o
    0x08000168   0x08000168   0x00000020   Code   RO         2974    .text               mc_w.l(llushr.o)
    0x08000188   0x08000188   0x00000024   Code   RO         2976    .text               mc_w.l(memcpya.o)
    0x080001ac   0x080001ac   0x00000024   Code   RO         2978    .text               mc_w.l(memseta.o)
    0x080001d0   0x080001d0   0x00000062   Code   RO         3260    .text               mc_w.l(uldiv.o)
    0x08000232   0x08000232   0x00000002   PAD
    0x08000234   0x08000234   0x00000024   Code   RO         3273    .text               mc_w.l(init.o)
    0x08000258   0x08000258   0x0000001e   Code   RO         3275    .text               mc_w.l(llshl.o)
    0x08000276   0x08000276   0x00000002   Code   RO          183    i.BusFault_Handler  stm32f1xx_it.o
    0x08000278   0x08000278   0x00000002   Code   RO          184    i.DebugMon_Handler  stm32f1xx_it.o
    0x0800027a   0x0800027a   0x00000002   PAD
    0x0800027c   0x0800027c   0x00000018   Code   RO         2303    i.DelayMs           timer.o
    0x08000294   0x08000294   0x00000006   Code   RO          185    i.EXTI0_IRQHandler  stm32f1xx_it.o
    0x0800029a   0x0800029a   0x00000002   PAD
    0x0800029c   0x0800029c   0x0000001c   Code   RO         2076    i.HAL_GPIO_EXTI_Callback  sx126x-board.o
    0x080002b8   0x080002b8   0x00000018   Code   RO          984    i.HAL_GPIO_EXTI_IRQHandler  stm32f1xx_hal_gpio.o
    0x080002d0   0x080002d0   0x000001f8   Code   RO          985    i.HAL_GPIO_Init     stm32f1xx_hal_gpio.o
    0x080004c8   0x080004c8   0x0000000a   Code   RO          987    i.HAL_GPIO_ReadPin  stm32f1xx_hal_gpio.o
    0x080004d2   0x080004d2   0x0000000a   Code   RO          989    i.HAL_GPIO_WritePin  stm32f1xx_hal_gpio.o
    0x080004dc   0x080004dc   0x0000000c   Code   RO          681    i.HAL_GetTick       stm32f1xx_hal.o
    0x080004e8   0x080004e8   0x00000010   Code   RO          687    i.HAL_IncTick       stm32f1xx_hal.o
    0x080004f8   0x080004f8   0x00000024   Code   RO          688    i.HAL_Init          stm32f1xx_hal.o
    0x0800051c   0x0800051c   0x00000040   Code   RO          689    i.HAL_InitTick      stm32f1xx_hal.o
    0x0800055c   0x0800055c   0x0000003c   Code   RO          264    i.HAL_MspInit       stm32f1xx_hal_msp.o
    0x08000598   0x08000598   0x00000022   Code   RO         1144    i.HAL_NVIC_DisableIRQ  stm32f1xx_hal_cortex.o
    0x080005ba   0x080005ba   0x0000001a   Code   RO         1145    i.HAL_NVIC_EnableIRQ  stm32f1xx_hal_cortex.o
    0x080005d4   0x080005d4   0x00000040   Code   RO         1151    i.HAL_NVIC_SetPriority  stm32f1xx_hal_cortex.o
    0x08000614   0x08000614   0x00000024   Code   RO         1152    i.HAL_NVIC_SetPriorityGrouping  stm32f1xx_hal_cortex.o
    0x08000638   0x08000638   0x0000012c   Code   RO          845    i.HAL_RCC_ClockConfig  stm32f1xx_hal_rcc.o
    0x08000764   0x08000764   0x00000020   Code   RO          852    i.HAL_RCC_GetPCLK1Freq  stm32f1xx_hal_rcc.o
    0x08000784   0x08000784   0x00000020   Code   RO          853    i.HAL_RCC_GetPCLK2Freq  stm32f1xx_hal_rcc.o
    0x080007a4   0x080007a4   0x0000006c   Code   RO          854    i.HAL_RCC_GetSysClockFreq  stm32f1xx_hal_rcc.o
    0x08000810   0x08000810   0x00000320   Code   RO          857    i.HAL_RCC_OscConfig  stm32f1xx_hal_rcc.o
    0x08000b30   0x08000b30   0x000000b2   Code   RO          359    i.HAL_SPI_Init      stm32f1xx_hal_spi.o
    0x08000be2   0x08000be2   0x00000002   PAD
    0x08000be4   0x08000be4   0x00000070   Code   RO          266    i.HAL_SPI_MspInit   stm32f1xx_hal_msp.o
    0x08000c54   0x08000c54   0x00000166   Code   RO          367    i.HAL_SPI_Transmit  stm32f1xx_hal_spi.o
    0x08000dba   0x08000dba   0x000001e2   Code   RO          368    i.HAL_SPI_TransmitReceive  stm32f1xx_hal_spi.o
    0x08000f9c   0x08000f9c   0x00000028   Code   RO         1156    i.HAL_SYSTICK_Config  stm32f1xx_hal_cortex.o
    0x08000fc4   0x08000fc4   0x00000062   Code   RO         1710    i.HAL_UART_Init     stm32f1xx_hal_uart.o
    0x08001026   0x08001026   0x00000002   PAD
    0x08001028   0x08001028   0x00000070   Code   RO          268    i.HAL_UART_MspInit  stm32f1xx_hal_msp.o
    0x08001098   0x08001098   0x000000b2   Code   RO         1718    i.HAL_UART_Transmit  stm32f1xx_hal_uart.o
    0x0800114a   0x0800114a   0x00000002   Code   RO          186    i.HardFault_Handler  stm32f1xx_it.o
    0x0800114c   0x0800114c   0x0000016c   Code   RO         2904    i.LoRa_Init         test.o
    0x080012b8   0x080012b8   0x00000134   Code   RO         2905    i.LoRa_Test_Handle  test.o
    0x080013ec   0x080013ec   0x00000030   Code   RO         2906    i.LoRa_Test_Main    test.o
    0x0800141c   0x0800141c   0x000000d4   Code   RO           14    i.MX_GPIO_Init      main.o
    0x080014f0   0x080014f0   0x00000044   Code   RO           15    i.MX_SPI1_Init      main.o
    0x08001534   0x08001534   0x00000002   Code   RO          187    i.MemManage_Handler  stm32f1xx_it.o
    0x08001536   0x08001536   0x00000002   Code   RO          188    i.NMI_Handler       stm32f1xx_it.o
    0x08001538   0x08001538   0x00000080   Code   RO         2907    i.OnRxDone          test.o
    0x080015b8   0x080015b8   0x00000024   Code   RO         2908    i.OnRxError         test.o
    0x080015dc   0x080015dc   0x00000024   Code   RO         2909    i.OnRxTimeout       test.o
    0x08001600   0x08001600   0x00000024   Code   RO         2910    i.OnTxDone          test.o
    0x08001624   0x08001624   0x00000024   Code   RO         2911    i.OnTxTimeout       test.o
    0x08001648   0x08001648   0x00000002   Code   RO          189    i.PendSV_Handler    stm32f1xx_it.o
    0x0800164a   0x0800164a   0x00000002   PAD
    0x0800164c   0x0800164c   0x0000005c   Code   RO         2372    i.RadioAddRegisterToRetentionList  radio.o
    0x080016a8   0x080016a8   0x00000004   Code   RO         2373    i.RadioCheckRfFrequency  radio.o
    0x080016ac   0x080016ac   0x00000034   Code   RO         2374    i.RadioGetFskBandwidthRegValue  radio.o
    0x080016e0   0x080016e0   0x0000007a   Code   RO         2375    i.RadioGetLoRaTimeOnAirNumerator  radio.o
    0x0800175a   0x0800175a   0x00000022   Code   RO         2376    i.RadioGetStatus    radio.o
    0x0800177c   0x0800177c   0x0000000a   Code   RO         2377    i.RadioGetWakeupTime  radio.o
    0x08001786   0x08001786   0x00000002   PAD
    0x08001788   0x08001788   0x00000074   Code   RO         2378    i.RadioInit         radio.o
    0x080017fc   0x080017fc   0x00000150   Code   RO         2379    i.RadioIrqProcess   radio.o
    0x0800194c   0x0800194c   0x0000007a   Code   RO         2380    i.RadioIsChannelFree  radio.o
    0x080019c6   0x080019c6   0x00000002   PAD
    0x080019c8   0x080019c8   0x0000000c   Code   RO         2381    i.RadioOnDioIrq     radio.o
    0x080019d4   0x080019d4   0x00000018   Code   RO         2382    i.RadioOnRxTimeoutIrq  radio.o
    0x080019ec   0x080019ec   0x00000018   Code   RO         2383    i.RadioOnTxTimeoutIrq  radio.o
    0x08001a04   0x08001a04   0x0000001c   Code   RO         2384    i.RadioRandom       radio.o
    0x08001a20   0x08001a20   0x00000006   Code   RO         2385    i.RadioRead         radio.o
    0x08001a26   0x08001a26   0x00000006   Code   RO         2386    i.RadioReadBuffer   radio.o
    0x08001a2c   0x08001a2c   0x00000004   Code   RO         2387    i.RadioRssi         radio.o
    0x08001a30   0x08001a30   0x00000044   Code   RO         2388    i.RadioRx           radio.o
    0x08001a74   0x08001a74   0x00000044   Code   RO         2389    i.RadioRxBoosted    radio.o
    0x08001ab8   0x08001ab8   0x00000058   Code   RO         2390    i.RadioSend         radio.o
    0x08001b10   0x08001b10   0x00000004   Code   RO         2391    i.RadioSetChannel   radio.o
    0x08001b14   0x08001b14   0x00000028   Code   RO         2392    i.RadioSetMaxPayloadLength  radio.o
    0x08001b3c   0x08001b3c   0x00000030   Code   RO         2393    i.RadioSetModem     radio.o
    0x08001b6c   0x08001b6c   0x00000038   Code   RO         2394    i.RadioSetPublicNetwork  radio.o
    0x08001ba4   0x08001ba4   0x000001b4   Code   RO         2395    i.RadioSetRxConfig  radio.o
    0x08001d58   0x08001d58   0x00000004   Code   RO         2396    i.RadioSetRxDutyCycle  radio.o
    0x08001d5c   0x08001d5c   0x00000170   Code   RO         2397    i.RadioSetTxConfig  radio.o
    0x08001ecc   0x08001ecc   0x00000030   Code   RO         2398    i.RadioSetTxContinuousWave  radio.o
    0x08001efc   0x08001efc   0x00000012   Code   RO         2399    i.RadioSleep        radio.o
    0x08001f0e   0x08001f0e   0x00000006   Code   RO         2400    i.RadioStandby      radio.o
    0x08001f14   0x08001f14   0x00000018   Code   RO         2401    i.RadioStartCad     radio.o
    0x08001f2c   0x08001f2c   0x000000cc   Code   RO         2402    i.RadioTimeOnAir    radio.o
    0x08001ff8   0x08001ff8   0x00000006   Code   RO         2403    i.RadioWrite        radio.o
    0x08001ffe   0x08001ffe   0x00000006   Code   RO         2404    i.RadioWriteBuffer  radio.o
    0x08002004   0x08002004   0x00000020   Code   RO          397    i.SPI_EndRxTxTransaction  stm32f1xx_hal_spi.o
    0x08002024   0x08002024   0x000000b8   Code   RO          402    i.SPI_WaitFlagStateUntilTimeout  stm32f1xx_hal_spi.o
    0x080020dc   0x080020dc   0x00000002   Code   RO          190    i.SVC_Handler       stm32f1xx_it.o
    0x080020de   0x080020de   0x00000002   Code   RO         2077    i.SX126xAntSwOff    sx126x-board.o
    0x080020e0   0x080020e0   0x00000002   Code   RO         2078    i.SX126xAntSwOn     sx126x-board.o
    0x080020e2   0x080020e2   0x00000002   PAD
    0x080020e4   0x080020e4   0x00000074   Code   RO         2606    i.SX126xCalibrateImage  sx126x.o
    0x08002158   0x08002158   0x00000020   Code   RO         2607    i.SX126xCheckDeviceReady  sx126x.o
    0x08002178   0x08002178   0x00000018   Code   RO         2609    i.SX126xClearIrqStatus  sx126x.o
    0x08002190   0x08002190   0x0000001e   Code   RO         2610    i.SX126xConvertFreqInHzToPllStep  sx126x.o
    0x080021ae   0x080021ae   0x00000002   PAD
    0x080021b0   0x080021b0   0x00000018   Code   RO         2082    i.SX126xDbgPinRxWrite  sx126x-board.o
    0x080021c8   0x080021c8   0x00000018   Code   RO         2083    i.SX126xDbgPinTxWrite  sx126x-board.o
    0x080021e0   0x080021e0   0x00000004   Code   RO         2084    i.SX126xGetBoardTcxoWakeupTime  sx126x-board.o
    0x080021e4   0x080021e4   0x00000004   Code   RO         2085    i.SX126xGetDeviceId  sx126x-board.o
    0x080021e8   0x080021e8   0x00000018   Code   RO         2086    i.SX126xGetDio1PinState  sx126x-board.o
    0x08002200   0x08002200   0x00000014   Code   RO         2612    i.SX126xGetIrqStatus  sx126x.o
    0x08002214   0x08002214   0x0000000c   Code   RO         2087    i.SX126xGetOperatingMode  sx126x-board.o
    0x08002220   0x08002220   0x00000070   Code   RO         2613    i.SX126xGetPacketStatus  sx126x.o
    0x08002290   0x08002290   0x0000000c   Code   RO         2614    i.SX126xGetPacketType  sx126x.o
    0x0800229c   0x0800229c   0x0000002e   Code   RO         2615    i.SX126xGetPayload  sx126x.o
    0x080022ca   0x080022ca   0x0000005e   Code   RO         2616    i.SX126xGetRandom   sx126x.o
    0x08002328   0x08002328   0x00000018   Code   RO         2617    i.SX126xGetRssiInst  sx126x.o
    0x08002340   0x08002340   0x0000003c   Code   RO         2618    i.SX126xGetRxBufferStatus  sx126x.o
    0x0800237c   0x0800237c   0x00000038   Code   RO         2620    i.SX126xInit        sx126x.o
    0x080023b4   0x080023b4   0x000000ac   Code   RO         2090    i.SX126xIoInit      sx126x-board.o
    0x08002460   0x08002460   0x0000002c   Code   RO         2091    i.SX126xIoIrqInit   sx126x-board.o
    0x0800248c   0x0800248c   0x00000006   Code   RO         2092    i.SX126xIoRfSwitchInit  sx126x-board.o
    0x08002492   0x08002492   0x00000002   Code   RO         2093    i.SX126xIoTcxoInit  sx126x-board.o
    0x08002494   0x08002494   0x0000006c   Code   RO         2094    i.SX126xReadBuffer  sx126x-board.o
    0x08002500   0x08002500   0x00000068   Code   RO         2095    i.SX126xReadCommand  sx126x-board.o
    0x08002568   0x08002568   0x00000010   Code   RO         2096    i.SX126xReadRegister  sx126x-board.o
    0x08002578   0x08002578   0x00000074   Code   RO         2097    i.SX126xReadRegisters  sx126x-board.o
    0x080025ec   0x080025ec   0x00000034   Code   RO         2098    i.SX126xReset       sx126x-board.o
    0x08002620   0x08002620   0x00000012   Code   RO         2621    i.SX126xSendPayload  sx126x.o
    0x08002632   0x08002632   0x00000016   Code   RO         2622    i.SX126xSetBufferBaseAddress  sx126x.o
    0x08002648   0x08002648   0x00000016   Code   RO         2623    i.SX126xSetCad      sx126x.o
    0x0800265e   0x0800265e   0x00000002   PAD
    0x08002660   0x08002660   0x00000028   Code   RO         2625    i.SX126xSetCrcPolynomial  sx126x.o
    0x08002688   0x08002688   0x00000028   Code   RO         2626    i.SX126xSetCrcSeed  sx126x.o
    0x080026b0   0x080026b0   0x0000000e   Code   RO         2627    i.SX126xSetDio2AsRfSwitchCtrl  sx126x.o
    0x080026be   0x080026be   0x00000036   Code   RO         2629    i.SX126xSetDioIrqParams  sx126x.o
    0x080026f4   0x080026f4   0x00000052   Code   RO         2631    i.SX126xSetLoRaSymbNumTimeout  sx126x.o
    0x08002746   0x08002746   0x00000002   PAD
    0x08002748   0x08002748   0x0000008c   Code   RO         2632    i.SX126xSetModulationParams  sx126x.o
    0x080027d4   0x080027d4   0x00000038   Code   RO         2099    i.SX126xSetOperatingMode  sx126x-board.o
    0x0800280c   0x0800280c   0x0000001e   Code   RO         2633    i.SX126xSetPaConfig  sx126x.o
    0x0800282a   0x0800282a   0x00000002   PAD
    0x0800282c   0x0800282c   0x000000c4   Code   RO         2634    i.SX126xSetPacketParams  sx126x.o
    0x080028f0   0x080028f0   0x0000001c   Code   RO         2635    i.SX126xSetPacketType  sx126x.o
    0x0800290c   0x0800290c   0x0000000a   Code   RO         2636    i.SX126xSetPayload  sx126x.o
    0x08002916   0x08002916   0x0000000e   Code   RO         2637    i.SX126xSetRegulatorMode  sx126x.o
    0x08002924   0x08002924   0x00000040   Code   RO         2638    i.SX126xSetRfFrequency  sx126x.o
    0x08002964   0x08002964   0x00000006   Code   RO         2100    i.SX126xSetRfTxPower  sx126x-board.o
    0x0800296a   0x0800296a   0x00000030   Code   RO         2639    i.SX126xSetRx       sx126x.o
    0x0800299a   0x0800299a   0x00000030   Code   RO         2640    i.SX126xSetRxBoosted  sx126x.o
    0x080029ca   0x080029ca   0x00000034   Code   RO         2641    i.SX126xSetRxDutyCycle  sx126x.o
    0x080029fe   0x080029fe   0x00000002   PAD
    0x08002a00   0x08002a00   0x00000040   Code   RO         2643    i.SX126xSetSleep    sx126x.o
    0x08002a40   0x08002a40   0x0000001e   Code   RO         2644    i.SX126xSetStandby  sx126x.o
    0x08002a5e   0x08002a5e   0x0000000e   Code   RO         2645    i.SX126xSetStopRxTimerOnPreambleDetect  sx126x.o
    0x08002a6c   0x08002a6c   0x00000012   Code   RO         2646    i.SX126xSetSyncWord  sx126x.o
    0x08002a7e   0x08002a7e   0x00000026   Code   RO         2647    i.SX126xSetTx       sx126x.o
    0x08002aa4   0x08002aa4   0x00000016   Code   RO         2648    i.SX126xSetTxContinuousWave  sx126x.o
    0x08002aba   0x08002aba   0x0000007e   Code   RO         2650    i.SX126xSetTxParams  sx126x.o
    0x08002b38   0x08002b38   0x00000038   Code   RO         2651    i.SX126xSetWhiteningSeed  sx126x.o
    0x08002b70   0x08002b70   0x00000018   Code   RO         2101    i.SX126xWaitOnBusy  sx126x-board.o
    0x08002b88   0x08002b88   0x0000004c   Code   RO         2102    i.SX126xWakeup      sx126x-board.o
    0x08002bd4   0x08002bd4   0x00000058   Code   RO         2103    i.SX126xWriteBuffer  sx126x-board.o
    0x08002c2c   0x08002c2c   0x0000005c   Code   RO         2104    i.SX126xWriteCommand  sx126x-board.o
    0x08002c88   0x08002c88   0x0000000c   Code   RO         2105    i.SX126xWriteRegister  sx126x-board.o
    0x08002c94   0x08002c94   0x00000060   Code   RO         2106    i.SX126xWriteRegisters  sx126x-board.o
    0x08002cf4   0x08002cf4   0x00000004   Code   RO          191    i.SysTick_Handler   stm32f1xx_it.o
    0x08002cf8   0x08002cf8   0x0000005c   Code   RO           16    i.SystemClock_Config  main.o
    0x08002d54   0x08002d54   0x00000002   Code   RO         2039    i.SystemInit        system_stm32f1xx.o
    0x08002d56   0x08002d56   0x00000004   Code   RO         2304    i.TimerGetCurrentTime  timer.o
    0x08002d5a   0x08002d5a   0x0000000c   Code   RO         2305    i.TimerGetElapsedTime  timer.o
    0x08002d66   0x08002d66   0x00000002   PAD
    0x08002d68   0x08002d68   0x0000002c   Code   RO         2306    i.TimerInit         timer.o
    0x08002d94   0x08002d94   0x00000050   Code   RO         2307    i.TimerService      timer.o
    0x08002de4   0x08002de4   0x0000000c   Code   RO         2308    i.TimerSetValue     timer.o
    0x08002df0   0x08002df0   0x00000018   Code   RO         2309    i.TimerStart        timer.o
    0x08002e08   0x08002e08   0x0000000a   Code   RO         2310    i.TimerStop         timer.o
    0x08002e12   0x08002e12   0x00000002   PAD
    0x08002e14   0x08002e14   0x000000b8   Code   RO         1736    i.UART_SetConfig    stm32f1xx_hal_uart.o
    0x08002ecc   0x08002ecc   0x00000064   Code   RO         1739    i.UART_WaitOnFlagUntilTimeout  stm32f1xx_hal_uart.o
    0x08002f30   0x08002f30   0x00000002   Code   RO          192    i.UsageFault_Handler  stm32f1xx_it.o
    0x08002f32   0x08002f32   0x00000002   PAD
    0x08002f34   0x08002f34   0x00000020   Code   RO         3189    i.__0printf$8       mc_w.l(printf8.o)
    0x08002f54   0x08002f54   0x00000020   Code   RO         1158    i.__NVIC_SetPriority  stm32f1xx_hal_cortex.o
    0x08002f74   0x08002f74   0x0000000e   Code   RO         3283    i.__scatterload_copy  mc_w.l(handlers.o)
    0x08002f82   0x08002f82   0x00000002   Code   RO         3284    i.__scatterload_null  mc_w.l(handlers.o)
    0x08002f84   0x08002f84   0x0000000e   Code   RO         3285    i.__scatterload_zeroinit  mc_w.l(handlers.o)
    0x08002f92   0x08002f92   0x00000002   PAD
    0x08002f94   0x08002f94   0x00000410   Code   RO         3196    i._printf_core      mc_w.l(printf8.o)
    0x080033a4   0x080033a4   0x00000024   Code   RO         3197    i._printf_post_padding  mc_w.l(printf8.o)
    0x080033c8   0x080033c8   0x0000002e   Code   RO         3198    i._printf_pre_padding  mc_w.l(printf8.o)
    0x080033f6   0x080033f6   0x00000002   PAD
    0x080033f8   0x080033f8   0x0000001c   Code   RO           17    i.fputc             main.o
    0x08003414   0x08003414   0x00000060   Code   RO           18    i.main              main.o
    0x08003474   0x08003474   0x00000010   Data   RO         2040    .constdata          system_stm32f1xx.o
    0x08003484   0x08003484   0x00000008   Data   RO         2041    .constdata          system_stm32f1xx.o
    0x0800348c   0x0800348c   0x0000006c   Data   RO         2406    .constdata          radio.o
    0x080034f8   0x080034f8   0x000000b4   Data   RO         2407    .constdata          radio.o
    0x080035ac   0x080035ac   0x00000020   Data   RO         3281    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x20000000, Load base: 0x080035cc, Size: 0x00000ab8, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20000000   0x080035cc   0x0000000c   Data   RW          695    .data               stm32f1xx_hal.o
    0x2000000c   0x080035d8   0x00000004   Data   RW         2042    .data               system_stm32f1xx.o
    0x20000010   0x080035dc   0x00000008   Data   RW         2108    .data               sx126x-board.o
    0x20000018   0x080035e4   0x00000004   Data   RW         2312    .data               timer.o
    0x2000001c   0x080035e8   0x00000014   Data   RW         2408    .data               radio.o
    0x20000030   0x080035fc   0x00000008   Data   RW         2652    .data               sx126x.o
    0x20000038   0x08003604   0x00000001   Data   RW         2913    .data               test.o
    0x20000039   0x08003605   0x00000003   PAD
    0x2000003c   0x08003608   0x00000004   Data   RW         3257    .data               mc_w.l(stdout.o)
    0x20000040        -       0x0000009c   Zero   RW           19    .bss                main.o
    0x200000dc        -       0x00000208   Zero   RW         2107    .bss                sx126x-board.o
    0x200002e4        -       0x00000018   Zero   RW         2311    .bss                timer.o
    0x200002fc        -       0x00000180   Zero   RW         2405    .bss                radio.o
    0x2000047c        -       0x0000023c   Zero   RW         2912    .bss                test.o
    0x200006b8        -       0x00000400   Zero   RW            1    STACK               startup_stm32f103xe.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

       496         56          0          0        156     474679   main.o
      2484        176        288         20        384      25828   radio.o
        36          8        304          0       1024        800   startup_stm32f103xe.o
       128         24          0         12          0       5885   stm32f1xx_hal.o
       232         14          0          0          0      29601   stm32f1xx_hal_cortex.o
       548         48          0          0          0       4118   stm32f1xx_hal_gpio.o
       284         34          0          0          0       2207   stm32f1xx_hal_msp.o
      1272        100          0          0          0       5188   stm32f1xx_hal_rcc.o
      1234          4          0          0          0       6184   stm32f1xx_hal_spi.o
       560          6          0          0          0       3936   stm32f1xx_hal_uart.o
        26          0          0          0          0       4205   stm32f1xx_it.o
      1194        172          0          8        520      23104   sx126x-board.o
      1916         82          0          8          0      24010   sx126x.o
         2          0         24          4          0       1087   system_stm32f1xx.o
       992        468          0          1        572       5344   test.o
       210         16          0          4         24       4742   timer.o

    ----------------------------------------------------------------------
     11646       1208        648         60       2680     620918   Object Totals
         0          0         32          0          0          0   (incl. Generated)
        32          0          0          3          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        36          8          0          0          0         68   init.o
        30          0          0          0          0         68   llshl.o
        32          0          0          0          0         68   llushr.o
        36          0          0          0          0         68   memcpya.o
        36          0          0          0          0        108   memseta.o
      1154         54          0          0          0        352   printf8.o
         0          0          0          4          0          0   stdout.o
        98          0          0          0          0         92   uldiv.o

    ----------------------------------------------------------------------
      1478         70          0          4          0        824   Library Totals
         6          0          0          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

      1472         70          0          4          0        824   mc_w.l

    ----------------------------------------------------------------------
      1478         70          0          4          0        824   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     13124       1278        648         64       2680     613470   Grand Totals
     13124       1278        648         64       2680     613470   ELF Image Totals
     13124       1278        648         64          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                13772 (  13.45kB)
    Total RW  Size (RW Data + ZI Data)              2744 (   2.68kB)
    Total ROM Size (Code + RO Data + RW Data)      13836 (  13.51kB)

==============================================================================

