Static Call Graph - [STM32L4_OneNET\STM32L4_OneNET.axf]

# Static Call Graph for image STM32L4_OneNET\STM32L4_OneNET.axf

#<CALLGRAPH># ARM Linker, 5060422: Last Updated: Fri Jun 22 16:10:54 2018

### Maximum Stack Usage = 296 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLLSAI2_Config

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- Error_Handler ⇒ Error_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - ADC3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - BusFault_Handler from stm32l4xx_it.o(i.BusFault_Handler) referenced from startup_stm32l476xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - COMP_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DFSDM1_FLT0_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DFSDM1_FLT1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DFSDM1_FLT2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DFSDM1_FLT3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA1_Channel4_IRQHandler from stm32l4xx_it.o(i.DMA1_Channel4_IRQHandler) referenced from startup_stm32l476xx.o(RESET)
  - DMA1_Channel5_IRQHandler from stm32l4xx_it.o(i.DMA1_Channel5_IRQHandler) referenced from startup_stm32l476xx.o(RESET)
  - DMA1_Channel6_IRQHandler from stm32l4xx_it.o(i.DMA1_Channel6_IRQHandler) referenced from startup_stm32l476xx.o(RESET)
  - DMA1_Channel7_IRQHandler from stm32l4xx_it.o(i.DMA1_Channel7_IRQHandler) referenced from startup_stm32l476xx.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA2_Channel6_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DMA2_Channel7_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - DebugMon_Handler from stm32l4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32l476xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - FMC_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - FPU_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - HardFault_Handler from stm32l4xx_it.o(i.HardFault_Handler) referenced from startup_stm32l476xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - LCD_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - LPTIM1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - LPTIM2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - LPUART1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - MemManage_Handler from stm32l4xx_it.o(i.MemManage_Handler) referenced from startup_stm32l476xx.o(RESET)
  - NMI_Handler from stm32l4xx_it.o(i.NMI_Handler) referenced from startup_stm32l476xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - PVD_PVM_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - PendSV_Handler from stm32l4xx_it.o(i.PendSV_Handler) referenced from startup_stm32l476xx.o(RESET)
  - QUADSPI_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - RCC_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - RNG_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - Reset_Handler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SAI2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SDMMC1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SVC_Handler from stm32l4xx_it.o(i.SVC_Handler) referenced from startup_stm32l476xx.o(RESET)
  - SWPMI1_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - SysTick_Handler from stm32l4xx_it.o(i.SysTick_Handler) referenced from startup_stm32l476xx.o(RESET)
  - SystemInit from system_stm32l4xx.o(i.SystemInit) referenced from startup_stm32l476xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM1_BRK_TIM15_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM1_TRG_COM_TIM17_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM1_UP_TIM16_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - TSC_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - UART4_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - UART5_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - UART_DMAAbortOnError from stm32l4xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32l4xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - UART_DMAError from stm32l4xx_hal_uart.o(i.UART_DMAError) referenced from stm32l4xx_hal_uart.o(i.HAL_UART_Receive_DMA)
  - UART_DMAError from stm32l4xx_hal_uart.o(i.UART_DMAError) referenced from stm32l4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)
  - UART_DMAReceiveCplt from stm32l4xx_hal_uart.o(i.UART_DMAReceiveCplt) referenced from stm32l4xx_hal_uart.o(i.HAL_UART_Receive_DMA)
  - UART_DMARxHalfCplt from stm32l4xx_hal_uart.o(i.UART_DMARxHalfCplt) referenced from stm32l4xx_hal_uart.o(i.HAL_UART_Receive_DMA)
  - UART_DMATransmitCplt from stm32l4xx_hal_uart.o(i.UART_DMATransmitCplt) referenced from stm32l4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)
  - UART_DMATxHalfCplt from stm32l4xx_hal_uart.o(i.UART_DMATxHalfCplt) referenced from stm32l4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)
  - USART1_IRQHandler from stm32l4xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32l476xx.o(RESET)
  - USART2_IRQHandler from stm32l4xx_it.o(i.USART2_IRQHandler) referenced from startup_stm32l476xx.o(RESET)
  - USART3_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - UsageFault_Handler from stm32l4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32l476xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32l476xx.o(.text) referenced from startup_stm32l476xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32l476xx.o(.text)
  - _sputc from printf3.o(i._sputc) referenced from printf3.o(i.__0sprintf$3)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  COMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DFSDM1_FLT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DFSDM1_FLT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DFSDM1_FLT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DFSDM1_FLT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA2_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  DMA2_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  LPTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  LPTIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  LPUART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  PVD_PVM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  QUADSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SAI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SDMMC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SWPMI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM1_BRK_TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM1_TRG_COM_TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM1_UP_TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32l476xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> UART_SetConfig

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> nb73_task

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strstr (Thumb, 36 bytes, Stack size 12 bytes, strstr.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strstr
  [Called By]
  - >> NB73_get_id
  - >> nb73_task

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> nb73_task
  - >> uart_send_stream

  atoi (Thumb, 26 bytes, Stack size 16 bytes, atoi.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> strtol
  - >> __aeabi_errno_addr
  [Called By]
  - >> NB73_get_id

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  strtol (Thumb, 112 bytes, Stack size 32 bytes, strtol.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = strtol ⇒ _strtoul
  [Calls]
  - >> _strtoul
  - >> __rt_ctype_table
  - >> __aeabi_errno_addr
  [Called By]
  - >> atoi

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __rt_ctype_table (Thumb, 4 bytes, Stack size 0 bytes, ctype_o.o(.text))
  [Called By]

  - >> strtol

  _strtoul (Thumb, 158 bytes, Stack size 40 bytes, _strtoul.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _strtoul
  [Calls]
  - >> _chval
  - >> __aeabi_errno_addr
  [Called By]
  - >> strtol

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _strtoul

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.DMA1_Channel4_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA1_Channel4_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.DMA1_Channel5_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA1_Channel5_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.DMA1_Channel6_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA1_Channel6_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.DMA1_Channel7_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA1_Channel7_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  Error_Handler (Thumb, 2 bytes, Stack size 0 bytes, main.o(i.Error_Handler))
  [Calls]

  - >> Error_Handler
  [Called By]
  - >> MX_TIM1_Init
  - >> Error_Handler
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  - >> HAL_UART_MspInit

  HAL_DMA_Abort (Thumb, 68 bytes, Stack size 8 bytes, stm32l4xx_hal_dma.o(i.HAL_DMA_Abort))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort
  [Called By]
  - >> HAL_UART_AbortReceive

  HAL_DMA_Abort_IT (Thumb, 74 bytes, Stack size 8 bytes, stm32l4xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_IRQHandler (Thumb, 168 bytes, Stack size 16 bytes, stm32l4xx_hal_dma.o(i.HAL_DMA_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_IRQHandler
  [Called By]
  - >> DMA1_Channel7_IRQHandler
  - >> DMA1_Channel6_IRQHandler
  - >> DMA1_Channel5_IRQHandler
  - >> DMA1_Channel4_IRQHandler

  HAL_DMA_Init (Thumb, 178 bytes, Stack size 16 bytes, stm32l4xx_hal_dma.o(i.HAL_DMA_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_Init
  [Called By]
  - >> HAL_UART_MspInit

  HAL_DMA_Start_IT (Thumb, 112 bytes, Stack size 16 bytes, stm32l4xx_hal_dma.o(i.HAL_DMA_Start_IT))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> DMA_SetConfig
  [Called By]
  - >> HAL_UART_Transmit_DMA
  - >> HAL_UART_Receive_DMA

  HAL_Delay (Thumb, 28 bytes, Stack size 16 bytes, stm32l4xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> nb73_task
  - >> uart_send_stream

  HAL_GPIO_Init (Thumb, 414 bytes, Stack size 40 bytes, stm32l4xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> dht11_gpio_output
  - >> dht11_gpio_input
  - >> MX_GPIO_Init
  - >> HAL_UART_MspInit

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32l4xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> dht11_scan
  - >> dht11_read_bit

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32l4xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> dht11_reset
  - >> turn_on_led
  - >> turn_off_led
  - >> MX_GPIO_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32l4xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> UART_WaitOnFlagUntilTimeout
  - >> UART_CheckIdleState
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> RCCEx_PLLSAI2_Config
  - >> RCCEx_PLLSAI1_Config
  - >> HAL_Delay
  - >> nb73_task

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32l4xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 22 bytes, Stack size 8 bytes, stm32l4xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32l4xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 122 bytes, Stack size 8 bytes, stm32l4xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32l4xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> MX_DMA_Init
  - >> HAL_UART_MspInit

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32l4xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> HAL_MspInit
  - >> MX_DMA_Init
  - >> SystemClock_Config
  - >> HAL_UART_MspInit

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32l4xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init
  - >> HAL_MspInit

  HAL_NVIC_SystemReset (Thumb, 26 bytes, Stack size 0 bytes, stm32l4xx_hal_cortex.o(i.HAL_NVIC_SystemReset))
  [Called By]

  - >> nb73_task

  HAL_PWREx_ControlVoltageScaling (Thumb, 86 bytes, Stack size 0 bytes, stm32l4xx_hal_pwr_ex.o(i.HAL_PWREx_ControlVoltageScaling))
  [Called By]

  - >> SystemClock_Config

  HAL_PWREx_GetVoltageRange (Thumb, 10 bytes, Stack size 0 bytes, stm32l4xx_hal_pwr_ex.o(i.HAL_PWREx_GetVoltageRange))
  [Called By]

  - >> RCC_SetFlashLatencyFromMSIRange

  HAL_RCCEx_PeriphCLKConfig (Thumb, 928 bytes, Stack size 40 bytes, stm32l4xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLLSAI2_Config
  [Calls]
  - >> HAL_GetTick
  - >> RCCEx_PLLSAI2_Config
  - >> RCCEx_PLLSAI1_Config
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 368 bytes, Stack size 32 bytes, stm32l4xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32l4xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 34 bytes, Stack size 0 bytes, stm32l4xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 34 bytes, Stack size 0 bytes, stm32l4xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 238 bytes, Stack size 16 bytes, stm32l4xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> UART_SetConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 1152 bytes, Stack size 32 bytes, stm32l4xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RCC_OscConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  - >> RCC_SetFlashLatencyFromMSIRange
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32l4xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32l4xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32l4xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 78 bytes, Stack size 12 bytes, stm32l4xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_Base_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32l4xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_Base_MspInit (Thumb, 30 bytes, Stack size 8 bytes, tim.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_Base_MspInit
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start (Thumb, 26 bytes, Stack size 0 bytes, stm32l4xx_hal_tim.o(i.HAL_TIM_Base_Start))
  [Called By]

  - >> delay_us

  HAL_TIM_Base_Stop (Thumb, 44 bytes, Stack size 0 bytes, stm32l4xx_hal_tim.o(i.HAL_TIM_Base_Stop))
  [Called By]

  - >> delay_us

  HAL_TIM_ConfigClockSource (Thumb, 246 bytes, Stack size 16 bytes, stm32l4xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_ETR_SetConfig
  [Calls]
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  [Called By]
  - >> MX_TIM1_Init

  HAL_UARTEx_WakeupCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_hal_uart_ex.o(i.HAL_UARTEx_WakeupCallback))
  [Called By]

  - >> HAL_UART_IRQHandler

  HAL_UART_AbortReceive (Thumb, 76 bytes, Stack size 16 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_AbortReceive))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_UART_AbortReceive ⇒ HAL_DMA_Abort
  [Calls]
  - >> HAL_DMA_Abort
  [Called By]
  - >> USART1_IRQHandler

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAError
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 408 bytes, Stack size 16 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_DMA_Abort_IT
  - >> HAL_UARTEx_WakeupCallback
  - >> HAL_UART_ErrorCallback
  - >> UART_Receive_IT
  - >> UART_EndRxTransfer
  - >> HAL_UART_TxCpltCallback
  [Called By]
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 106 bytes, Stack size 8 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  - >> HAL_UART_MspInit
  [Called By]
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init

  HAL_UART_MspInit (Thumb, 338 bytes, Stack size 56 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_DMA_Init
  - >> HAL_GPIO_Init
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> Error_Handler
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Receive_DMA (Thumb, 132 bytes, Stack size 16 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_Receive_DMA))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_UART_Receive_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  [Called By]
  - >> USART1_IRQHandler
  - >> main

  HAL_UART_RxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_RxCpltCallback))
  [Called By]

  - >> UART_Receive_IT
  - >> UART_DMAReceiveCplt

  HAL_UART_RxHalfCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_RxHalfCpltCallback))
  [Called By]

  - >> UART_DMARxHalfCplt

  HAL_UART_Transmit_DMA (Thumb, 122 bytes, Stack size 16 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_Transmit_DMA))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_UART_Transmit_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  [Called By]
  - >> uart_send_stream

  HAL_UART_TxCpltCallback (Thumb, 16 bytes, Stack size 0 bytes, usart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMATransmitCplt

  HAL_UART_TxHalfCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback))
  [Called By]

  - >> UART_DMATxHalfCplt

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  MX_DMA_Init (Thumb, 88 bytes, Stack size 8 bytes, dma.o(i.MX_DMA_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = MX_DMA_Init ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 106 bytes, Stack size 48 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> main

  MX_TIM1_Init (Thumb, 84 bytes, Stack size 40 bytes, tim.o(i.MX_TIM1_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_TIM1_Init ⇒ HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> Error_Handler
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 52 bytes, Stack size 8 bytes, usart.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_USART2_UART_Init (Thumb, 52 bytes, Stack size 8 bytes, usart.o(i.MX_USART2_UART_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_USART2_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  NB73_get_id (Thumb, 44 bytes, Stack size 16 bytes, wh-nb73.o(i.NB73_get_id))
  [Stack]

  - Max Depth = 104
  - Call Chain = NB73_get_id ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> atoi
  - >> strstr
  [Called By]
  - >> nb73_task

  NB73_onenet_init (Thumb, 50 bytes, Stack size 8 bytes, wh-nb73.o(i.NB73_onenet_init))
  [Stack]

  - Max Depth = 68
  - Call Chain = NB73_onenet_init ⇒ uart_send_stream ⇒ HAL_UART_Transmit_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> uart_send_stream
  [Called By]
  - >> nb73_task

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(RESET)

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32l4xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  SystemClock_Config (Thumb, 122 bytes, Stack size 232 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 296
  - Call Chain = SystemClock_Config ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLLSAI2_Config
  [Calls]
  - >> HAL_PWREx_ControlVoltageScaling
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> main

  SystemInit (Thumb, 56 bytes, Stack size 0 bytes, system_stm32l4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32l476xx.o(.text)

  TIM_Base_SetConfig (Thumb, 152 bytes, Stack size 32 bytes, stm32l4xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  TIM_ETR_SetConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32l4xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  UART_AdvFeatureConfig (Thumb, 200 bytes, Stack size 0 bytes, stm32l4xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Called By]

  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 92 bytes, Stack size 24 bytes, stm32l4xx_hal_uart.o(i.UART_CheckIdleState))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Init

  UART_SetConfig (Thumb, 614 bytes, Stack size 24 bytes, stm32l4xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 64
  - Call Chain = UART_SetConfig ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 100 bytes, Stack size 24 bytes, stm32l4xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> UART_CheckIdleState

  USART1_IRQHandler (Thumb, 70 bytes, Stack size 8 bytes, stm32l4xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 52
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_Receive_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_UART_Receive_DMA
  - >> HAL_UART_IRQHandler
  - >> HAL_UART_AbortReceive
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  USART2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART2_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32l4xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32l476xx.o(RESET)

  __0sprintf$3 (Thumb, 34 bytes, Stack size 24 bytes, printf3.o(i.__0sprintf$3), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$3 (Thumb, 0 bytes, Stack size 24 bytes, printf3.o(i.__0sprintf$3), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf3.o(i.__0sprintf$3))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> nb73_task

  __aeabi_errno_addr (Thumb, 4 bytes, Stack size 0 bytes, errno.o(i.__aeabi_errno_addr))
  [Called By]

  - >> _strtoul
  - >> strtol
  - >> atoi

  __rt_errno_addr (Thumb, 0 bytes, Stack size 0 bytes, errno.o(i.__aeabi_errno_addr), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  delay_us (Thumb, 38 bytes, Stack size 8 bytes, tim.o(i.delay_us))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_us
  [Calls]
  - >> HAL_TIM_Base_Stop
  - >> HAL_TIM_Base_Start
  [Called By]
  - >> dht11_reset
  - >> dht11_read_bit

  dht11_gpio_input (Thumb, 30 bytes, Stack size 24 bytes, dht11.o(i.dht11_gpio_input))
  [Stack]

  - Max Depth = 64
  - Call Chain = dht11_gpio_input ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> dht11_reset

  dht11_gpio_output (Thumb, 32 bytes, Stack size 24 bytes, dht11.o(i.dht11_gpio_output))
  [Stack]

  - Max Depth = 64
  - Call Chain = dht11_gpio_output ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> dht11_reset

  dht11_read_bit (Thumb, 56 bytes, Stack size 8 bytes, dht11.o(i.dht11_read_bit))
  [Stack]

  - Max Depth = 16
  - Call Chain = dht11_read_bit ⇒ delay_us
  [Calls]
  - >> HAL_GPIO_ReadPin
  - >> delay_us
  [Called By]
  - >> dht11_read_byte

  dht11_read_byte (Thumb, 32 bytes, Stack size 16 bytes, dht11.o(i.dht11_read_byte))
  [Stack]

  - Max Depth = 32
  - Call Chain = dht11_read_byte ⇒ dht11_read_bit ⇒ delay_us
  [Calls]
  - >> dht11_read_bit
  [Called By]
  - >> dht11_read_data

  dht11_read_data (Thumb, 90 bytes, Stack size 16 bytes, dht11.o(i.dht11_read_data))
  [Stack]

  - Max Depth = 88
  - Call Chain = dht11_read_data ⇒ dht11_reset ⇒ dht11_gpio_output ⇒ HAL_GPIO_Init
  [Calls]
  - >> dht11_scan
  - >> dht11_reset
  - >> dht11_read_byte
  [Called By]
  - >> nb73_task

  dht11_reset (Thumb, 52 bytes, Stack size 8 bytes, dht11.o(i.dht11_reset))
  [Stack]

  - Max Depth = 72
  - Call Chain = dht11_reset ⇒ dht11_gpio_output ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> dht11_gpio_output
  - >> dht11_gpio_input
  - >> delay_us
  [Called By]
  - >> dht11_read_data

  dht11_scan (Thumb, 10 bytes, Stack size 0 bytes, dht11.o(i.dht11_scan))
  [Calls]

  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> dht11_read_data

  get_led_state (Thumb, 6 bytes, Stack size 0 bytes, gpio.o(i.get_led_state))
  [Called By]

  - >> nb73_task

  main (Thumb, 70 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 296
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLLSAI2_Config
  [Calls]
  - >> HAL_UART_Receive_DMA
  - >> HAL_Init
  - >> nb73_task
  - >> MX_TIM1_Init
  - >> MX_DMA_Init
  - >> SystemClock_Config
  - >> turn_off_led
  - >> MX_GPIO_Init
  - >> uart_send_stream
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  nb73_task (Thumb, 844 bytes, Stack size 72 bytes, wh-nb73.o(i.nb73_task))
  [Stack]

  - Max Depth = 176
  - Call Chain = nb73_task ⇒ NB73_get_id ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> HAL_GetTick
  - >> HAL_NVIC_SystemReset
  - >> HAL_Delay
  - >> __2sprintf
  - >> strlen
  - >> strstr
  - >> __aeabi_memclr
  - >> NB73_onenet_init
  - >> NB73_get_id
  - >> dht11_read_data
  - >> turn_on_led
  - >> turn_off_led
  - >> get_led_state
  - >> uart_send_stream
  [Called By]
  - >> main

  turn_off_led (Thumb, 20 bytes, Stack size 8 bytes, gpio.o(i.turn_off_led))
  [Stack]

  - Max Depth = 8
  - Call Chain = turn_off_led
  [Calls]
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> nb73_task
  - >> main

  turn_on_led (Thumb, 20 bytes, Stack size 8 bytes, gpio.o(i.turn_on_led))
  [Stack]

  - Max Depth = 8
  - Call Chain = turn_on_led
  [Calls]
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> nb73_task

  uart_send_stream (Thumb, 68 bytes, Stack size 16 bytes, usart.o(i.uart_send_stream))
  [Stack]

  - Max Depth = 60
  - Call Chain = uart_send_stream ⇒ HAL_UART_Transmit_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_UART_Transmit_DMA
  - >> HAL_Delay
  - >> strlen
  [Called By]
  - >> NB73_onenet_init
  - >> nb73_task
  - >> main

  ### Local Symbols

  DMA_SetConfig (Thumb, 42 bytes, Stack size 12 bytes, stm32l4xx_hal_dma.o(i.DMA_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_SetConfig
  [Called By]
  - >> HAL_DMA_Start_IT

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32l4xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  UART_DMAAbortOnError (Thumb, 20 bytes, Stack size 8 bytes, stm32l4xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMAAbortOnError
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32l4xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_DMAError (Thumb, 74 bytes, Stack size 16 bytes, stm32l4xx_hal_uart.o(i.UART_DMAError))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMAError
  [Calls]
  - >> HAL_UART_ErrorCallback
  - >> UART_EndTxTransfer
  - >> UART_EndRxTransfer
  [Address Reference Count : 2]
  - stm32l4xx_hal_uart.o(i.HAL_UART_Receive_DMA)
  - stm32l4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)

  UART_DMAReceiveCplt (Thumb, 62 bytes, Stack size 8 bytes, stm32l4xx_hal_uart.o(i.UART_DMAReceiveCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMAReceiveCplt
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Address Reference Count : 1]
  - stm32l4xx_hal_uart.o(i.HAL_UART_Receive_DMA)

  UART_DMARxHalfCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32l4xx_hal_uart.o(i.UART_DMARxHalfCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMARxHalfCplt
  [Calls]
  - >> HAL_UART_RxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32l4xx_hal_uart.o(i.HAL_UART_Receive_DMA)

  UART_DMATransmitCplt (Thumb, 48 bytes, Stack size 8 bytes, stm32l4xx_hal_uart.o(i.UART_DMATransmitCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMATransmitCplt
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Address Reference Count : 1]
  - stm32l4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)

  UART_DMATxHalfCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32l4xx_hal_uart.o(i.UART_DMATxHalfCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMATxHalfCplt
  [Calls]
  - >> HAL_UART_TxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32l4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)

  UART_EndRxTransfer (Thumb, 28 bytes, Stack size 0 bytes, stm32l4xx_hal_uart.o(i.UART_EndRxTransfer))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAError

  UART_EndTxTransfer (Thumb, 18 bytes, Stack size 0 bytes, stm32l4xx_hal_uart.o(i.UART_EndTxTransfer))
  [Called By]

  - >> UART_DMAError

  UART_Receive_IT (Thumb, 118 bytes, Stack size 8 bytes, stm32l4xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  RCCEx_PLLSAI1_Config (Thumb, 342 bytes, Stack size 24 bytes, stm32l4xx_hal_rcc_ex.o(i.RCCEx_PLLSAI1_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCCEx_PLLSAI1_Config
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCCEx_PeriphCLKConfig

  RCCEx_PLLSAI2_Config (Thumb, 302 bytes, Stack size 24 bytes, stm32l4xx_hal_rcc_ex.o(i.RCCEx_PLLSAI2_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCCEx_PLLSAI2_Config
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCCEx_PeriphCLKConfig

  RCC_SetFlashLatencyFromMSIRange (Thumb, 116 bytes, Stack size 24 bytes, stm32l4xx_hal_rcc.o(i.RCC_SetFlashLatencyFromMSIRange))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_SetFlashLatencyFromMSIRange
  [Calls]
  - >> HAL_PWREx_GetVoltageRange
  [Called By]
  - >> HAL_RCC_OscConfig

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32l4xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_TI1_ConfigInputStage (Thumb, 34 bytes, Stack size 8 bytes, stm32l4xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 36 bytes, Stack size 8 bytes, stm32l4xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  _printf_core (Thumb, 436 bytes, Stack size 96 bytes, printf3.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  [Called By]
  - >> __0sprintf$3

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf3.o(i._sputc))
  [Called By]

  - >> __0sprintf$3
  [Address Reference Count : 1]
  - printf3.o(i.__0sprintf$3)

  ### Undefined Global Symbols